arXiv:1507.05488v2 [nucl-ex] 24 Jul 2015

The study of the thermal neutron flux in the deep underground laboratory DULB-4900^1

V.V. Alekseenko^†, Yu.M. Gavrilyuk^†, A.M. Gangapshev^†, A.M. Gezhaev^†, D.D. Dzhappuev^†, V.V. Kazalov^†, A.U. Kudzhaev^†, V.V. Kuzminov^†, S.I. Panasenko^‡, S.S. Ratkevich^‡, D.A. Tekueva^†, S.P. Yakimenko^†, Yu.V. Sten’kin^†

† Institute for Nuclear Research, RAS, Moscow, Russia ‡ Kharkiv National University, Kharkiv, Ukraine

Abstract We report on the study of thermal neutron flux using monitors based on mixture of ZnS(Ag) and LiF enriched with a lithium-6 isotope at the deep underground laboratory DULB-4900 at the Baksan Neutrino Observatory. An annual modulation of thermal neutron flux in DULB-4900 is observed. Experimental evidences were obtained of correlation between the long-term thermal neutron flux variations and the absolute humidity of the air in laboratory. The amplitude of the modulation exceed 5% of total neutron flux.

Keyword: Neutron background, Underground laboratory, Low-background measurements

1 Introduction

The characterization of the neutron fluence has become a critical issue for experiments that require these extreme low-background environments, such as ββ-decay, dark matter searches, and solar neutrino experiments [1, 2, 3]. As direct detection dark matter experiments seek to detect WIMP dark matter by observing nuclear recoils produced by WIMP interactions with nuclei, and as single scatter neutron events can produce nuclear recoils that are indistinguishable from WIMP interactions, the issue of in situ background control is particularly relevant in considering neutron backgrounds. Annual modulation of neutron flux in underground facilities could mimic annual modulation of signal from WIMPs, due to elastic scattering on nuclei of target. The neutron flux could depend on parameters such as humidity, temperature, pressure and other meteorological conditions. The long term measurement

1 Talk at The International Workshop on Prospects of Particle Physics: ”Neutrino Physics and Astrophysics” February 01 - Ferbuary 08, 2015, Valday, Russia of thermal neutron flux is performed to study these dependencies for underground facilities at the Baksan Neutrino Observatory of the Institute for Nuclear Researches Russian Academy of Science (BNO INR RAS) [4].

2 Experimental setup

The measurements are performed in box A1 of deep underground laboratory DULB-4900 (at a depth of 4900 m w.e., cosmic ray flux is reduced by a factor 10^7) [5]. Where the temperature of the air is ∼ 27^o C and is stable during the year. The experimental setup consist of four detectors (D1, D2, D3 and D4) and three sensors (temperature, humidity, pressure). The detectors are identical to that used in [6]. The schematic view of the setup is presented in Fig. 1. Each detector is an aluminium container with sizes 700 × 700 × 300 mm^3 which is viewed by photomultiplier tube (FEU-49), see Fig. 2. Thin scintillator made of solid granulated alloy^6LiF+ZnS(Ag) (∼ 3/1 in mass, thickness is ≃ 30 mg/cm^2) with the area of 600 × 600 mm^2 is placed on the bottom of the container. The reaction^6Li+n →^3H + α is used to detect thermal neutrons (Q=4.79 MeV, E_α = 2051 keV, E_H = 2735 keV, σ = 945 b at 300 K). The signals from each PMTs are splited after preamplifier, one goes to summator, another goes directly to input of digital oscilloscope. The signal after summator goes to input of digital oscilloscope as well. The sample of recorded signal is shown in Fig. 3. Each detector is an aluminium container with sizes 700 × 700 × 300 mm^3 which is viewed by photomultiplier tube (FEU-49), see Fig. 2. Thin scintillator made of solid granulated alloy^6LiF+ZnS(Ag) (∼ 3/1 in mass, thickness is ≃ 30 mg/cm^2) with the area of 600 × 600 mm^2 is placed on the bottom of the container. Detectors are similar to that proposed in [6]. The reaction^6Li+n →^3H + α is used to detect thermal neutrons (Q=4.79 MeV, E_α = 2051 keV, E_H = 2735 keV, σ = 945 b at 300 K). The signals from each PMTs are splited after preamplifier, one goes to summator, another goes directly to input of digital oscilloscope. The signal after summator goes to input of digital oscilloscope as well. The sample of recorded signal is shown in Fig. 3.

Between first and second stages, detectors were alternately calibrated with neutron source (n-source). n-source consisted of set of α-sources (^{238}Pu +^{239}Pu +^{226}Ra + triplet /^{233}U +^{238}Pu +^{239}Pu /, total activity - 131 kBq) covered with 0.1 mm beryllium foil. Sources were placed inside cylindrical polyethylene box. The thickness of the box wall is 5 cm. Neutrons come from reaction^9Be+α →^{12}C + n (Q=5.5 MeV, E_n ≃ 1 ÷ 8 MeV, σ ≃ 0.1 b, p_{α,n} ≃

Figure 1: Schematic view of the setup. PMT - photomultiplier, Σ - sumator, DO - digital oscilloscope, R - recorder, T - temperature sensor, H - humidity sensor, P - pressure sensor

Figure 2: Schematic view of the detector.

Figure 3: Pulse sample.

2.5 · 10^{−5}). Estimated activity of n-source is A_n ≃ 3.28 s^{−1} = 1.18 · 10^4 h^{−1}.

The n-source was attached to the bottom of detectors (close to the scintillator), so ∼ 50% of neutrons cross the scintillator. But only small part of neutrons are thermalised after passing 5 cm of polyethylene. Spectra collected with detector D1 are presented in Fig. 4 as example. The response of all detectors on n-source are similar, with increasing of count rate by 700 cts/day (see Fig. 5).

The difference in background count rate of detectors is due to different contamination of^{210}Pb in scintillators. Which appears in decay chain of 222Rn, when during production of scintillators daughter ions of^{222}Rn stick to the surface of the scintillator. The half-life of^{210}Pb is 22.3 y. It’s daughter nuclei^{210}Po decays due to α-decay inside the scintillator giving a signal similar to that from neutron detection. Assuming that detector D4 has no intrinsic background from^{210}Po we may conclude that sum count rate of all detectors from neutrons Φ_n ≤ 10400 cts/day at the beginning of calibration, rest Φ_r ≥ 7800 cts/day - intrinsic background from^{210}Po.

3 Results

First stage of the main measurements started 08 August 2012 y and finished 25 September 2013. Second stage started 06 November 2013, with additional elements in the setup: temperature, humidity and pressure sensors. In total,

Figure 4: Spectra from detector D1. Blue thin line - background plus nsource, motton blue line - background, red line - difference by n-source.

at the moment, we collected data for ≃ 2.7 years. The behaviour of the sum count rate of the detectors is presented in Fig. 6. The data, when all conditions were stable are used (ventilation system of tunnel is working well, gates are closed). The count rate is well fitted with cosine function with decreasing base line:

A = a · cos ( 2 · π · x b + c ) + d · x + e, (1)

where A - count rate [cts/day], x - time [day], a = 556, b = 356, c = −0.208, d = −0.736, e = 17949. So, the amplitude of neutron flux modulation ΔΦ_n ≥ 5% taking into account the intrinsic background from^{210}Po.

The behaviour of the count rate of the detectors and humidity is very similar to that measured in work [6]. The continuous decrease of count rate is due to decay of^{210}Pb. The maximums in count rate corresponds to summer, while minimum - winter. The explanation is, that the count rate depends on absolute humidity of the air in laboratory. Probably, humidity in air works as an additional moderator for neutrons coming from rock. The comparison of sum count rate of the setup with the humidity of the air in lab is presented in Fig. 7. It is well seen the strong correlation between count rate and humidity. In Fig. 8 the dependence of count rate from humidity of the air and fit result by linear function are shown. Thus, additional 1 g/m^3 of humidity in air gives a rise in sum count rate of detectors ΔΦ_n ≃ 500 cts/day.

Figure 5: Count rate of detectors during alternately calibration with nsource. Beginning of the calibration corresponds to ≃ 420 day in Fig. 6

This value is similar to amplitude of the annual modulation of count rate.

It is well seen the strong correlation between count rate and humidity. In Fig. 8 the dependence of count rate from humidity of the air and fit result by linear function are shown. Thus, additional 1 g/m^3 of humidity in air gives a rise in sum count rate of detectors ΔΦ_n ≃ 500 cts/day. This value is similar to amplitude of the annual modulation of count rate.

Another effect seen by our setup is, that in case of quick rise of humidity (for example ventilation of the tunnel is stopped) the count rate start to rise slowly (see Fig. 9). Assuming, that rise in count rate is 30 cts/h during 30 h and that additional humidity of 9 g/m^3 should give rise in count rate ΔΦ_n ≃ 190 cts/h, we may conclude, that it takes ≃ 190 h to get equilibrium. Such delay could be explained by humidification of the rock surface in the lab. It means two possible effect: 1 - better thermalization (moderation) of the neutrons from the bulk rock crossing cracks filled with water (humidity), 2 - higher albedo (reflection, refraction) of the neutrons incoming in to the rock, thus the lab with the humid wall works as a neutron trap. As result total flux of neutrons in the lab become higher.

Figure 6: Count rate of detectors during ∼ 2.7 years.

Figure 7: Count rate of the detectors and humidity during 1.5 y since 06 November 2013.

Figure 8: Correlation between count rate and humidity.

Figure 9: Effect of quick rise of humidity on count rate of the detectors.

4 Conclusion.

We performed long time measurement the background thermal neutron flux at underground laboratory DULB-4900 of BNO INR RAS, which is located at 3670 m from the entrance to underground facilities. Total time of measurements was equal to 2.7 years. The correlation of the counting rate of thermal neutrons with humidity (high humidity increases the neutron thermalization probability in air) was detected. An observed annual modulation of thermal neutron flux at DULB-4900 exceed 5% of total neutron flux. Such effects mean, that, for example, experiments looking for WIMPs should be carried out in a labs with walls covered by neutron shield (≃ 25 cm of polyethylene ≃ 2 mm of cadmium sheet, or equivalent).

The measurements are continuing.

The work was made in accordance with INR RAS plan of the Research and Developments.

References

[1] Gavrilyuk Yu.M., Gangapshev A.M., Kazalov V.V., et al., Indications of 2ν2K capture in^{78}Kr // Phys. Rev. C 2013. V.87, P.035501.

[2] Gavrilyuk Yu.M., Gangapshev A.M., Kazalov V.V., et al., First Result of the Experimental Search for the 2K-Capture of^{124}Xe with the Copper Proportional Counter // Physics of Particles and Nuclei, 2015, V.46, No.2, P.147.

[3] Gavrin V.N., The Russian-American gallium experiment SAGE // Phys. Usp. 2011. V.54 P.941.

[4] Kuzminov V.V., The Baksan Neutrino Observatory // Eur. Phys. J.

Plus 2012. V.127. P.113.

[5] Gavriljuk Ju.M., Gangapshev A.M., Gezhaev A.M. et al., Working characteristics of the New Low Background Laboratory (DULB-4900, Baksan Neutrino Observatory) // Nucl. Instr. Meth. A, 2013. V.729. P.576; arXiv: physics.ins-det/1204.6424; doi: 10.1016/j.nima.2013.07.090.

[6] Alekseenko V.V., Gavriluk Yu.M., Kuzminov V.V., and Stenkin Yu.V., Tidal effect in the radon-due neutron flux from the Earth’s crust // Journal of Physics: Conference Series 2010. V.203., 012045;