arXiv:1811.12805v1 [hep-ex] 26 Nov 2018

Jet Substructure Variables with the SiFCC Detector at 100 TeV

C.-H Yeh^{∗a},S.V. Chekanov^b ,A.V. Kotwal^c,J. Proudfoot^b,S. Sen^c,N.V. Tran^d,S.-S Yu^a aDepartment of Physics and Center for High Energy and High Field Physics, National Central University Chung-Li, Taoyuan City 32001, Taiwan bHEP Division, Argonne National Laboratory 9700 S. Cass Avenue, Argonne, IL 60439, USA cDepartment of Physics, Duke University Durham, NC 27708, USA dFermi National Accelerator Laboratory Batavia, IL 6051, USA E-mail: a9510130375@gmail.com, chekanov@anl.gov, kotwal@phy.duke.edu, proudfoot@anl.gov, sourav.sen@duke.edu, ntran@fnal.gov, syu@phy.ncu.edu.tw

Future experiments beyond the LHC era will measure high-momentum bosons (W , Z, H) and top quarks with strongly collimated decay products that form hadronic jets. This paper describes the studies of the performance of jet substructure variables using the Geant4 simulation of a detector designed for high energy pp collisions at a 100 TeV collider. The two-prong jets from Z^′ → WW and three-prong jets from Z^′ → tt̄ are compared with the background from light quark jets, assuming Z^′ masses in the range 5 – 40 TeV. Our results indicate that the performance of jetsubstructure reconstruction improves with reducing transverse cell sizes of a hadronic calorimeter from Δη × Δϕ = 0.087 × 0.087 to 0.022 × 0.022 in most cases.

The 39th International Conference on High Energy Physics (ICHEP2018) 4-11 July, 2018 Seoul, Korea

∗Speaker.

© Copyright owned by the author(s) under the terms of the Creative Commons Attribution-NonCommercial-NoDerivatives 4.0 International License (CC BY-NC-ND 4.0). https://pos.sissa.it/

Jet Substructure Variables with the SiFCC Detector at 100 TeV C.-H Yeh

Future high-energy experiments, such as FCC-hh and SppC, will measure high-momentum bosons (W , Z, H) and top quarks with strongly collimated decay products that form hadronic jets. This leads to many challenges for detector technologies. In particular, reconstruction of jet substructure variables for boosted jets with transverse momentum above 10 TeV requires appropriate cell sizes of hadronic calorimeters (HCALs). In order to estimate transverse segmentation of HCALs for very boosted objects at future experiments, we used a FCC-like detector geometry, a software based on Geant4 simulation and Monte Carlo event samples as described in [1].

In this study we simulated the Z^′ bosons with the mass of 5, 10, 20, and 40 TeV. These particles are forced to decay to two light-flavor jets (qq̄) as background and WW or tt̄ as signal, where W (→ qq̄) and t(→ W^+ b → qq̄b) decay hadronically. Using different configurations of HCAL geometry, we draw the receiver operating characteristic (ROC) curves to quantify the detector performance and find out the cell size that can give the best separation power to distinguish signal from background for different jet substructures.

We used several jet substructure variables, including jet soft-drop mass [2], N-subjettiness [3] and energy correlation function [4] in this study. The variables considered are τ_{21} and C^1_2 for the Z^′ → WW signal and τ_{32} for the Z^′ → tt̄ signal. Figure 1 shows the ROC curves for τ_{21} [3] using three HCAL cell sizes for jets with P_T ∼10 TeV. For the τ_{21} and C^1_2 variables, the Δη × Δϕ = 0.022 × 0.022 (or 5 × 5 cm^2) geometry gives optimal performance, while for the jet soft-drop mass variable, the Δη × Δϕ = 0.0043 × 0.0043 (or 1 × 1 cm^2) geometry gives optimal performance (followed by 5 × 5 cm^2). The results for the τ_{32} variable are inconclusive.

In conclusion, the performance of a HCAL with 5 × 5 cm^2 cells is, in most cases, better than for Δη × Δϕ = 0.087 × 0.087 (or 20 × 20 cm^2) cells. Therefore, this study confirms the baseline SiFCC detector geometry [1] that uses 5 × 5 cm^2 HCAL cells.

Figure 1: ROC curves for the τ_{21} substructure variable [3] for the decay Z^′ → WW with a Z^′ mass of 20 TeV. The calculations were performed for a HCAL with different transverse segmentations.

References

[1] S. V. Chekanov, M. Beydler, A. V. Kotwal, L. Gray, S. Sen, N. V. Tran, S.-S. Yu and J. Zuzelski, Initial performance studies of a general-purpose detector for multi-TeV physics at a 100 TeV pp collider, JINST 12, no. 06, P06009 (2017) doi:10.1088/1748-0221/12/06/P06009 [arXiv:1612.07291 [hep-ex]].

[2] A. J. Larkoski, S. Marzani, G. Soyez and J. Thaler, Soft Drop, JHEP 1405, 146 (2014) doi:10.1007/JHEP05(2014)146 [arXiv:1402.2657 [hep-ph]].

[3] J. Thaler and K. Van Tilburg, Identifying Boosted Objects with N-subjettiness, JHEP 1103, 015 (2011) doi:10.1007/JHEP03(2011)015 [arXiv:1011.2268 [hep-ph]].

[4] A. J. Larkoski, G. P. Salam and J. Thaler, Energy Correlation Functions for Jet Substructure, JHEP 1306, 108 (2013) doi:10.1007/JHEP06(2013)108 [arXiv:1305.0007 [hep-ph]]. 1