arXiv:2207.03272v2 [astro-ph.IM] 15 Jul 2022

Early results from GRBAlpha and VZLUSAT-2

Jakub Řípa^a, András Pál^b, Masanori Ohno^c, Norbert Werner^a, László Mészáros^b, Balázs Csák^b, Marianna Dafčíková^a, Vladimír Dániel^d, Juraj Dudáš^d, Marcel Frajt^e, Peter Hanák^f, Ján Hudec^e, Milan Junas^d, Jakub Kapuš^e, Miroslav Kasal^g, Martin Koleda^h, Robert Laszlo^h, Pavol Lipovský^f, Filip Münz^a, Maksim Rezenov^e, Miroslav Šmelko^f, Petr Svoboda^d, Hiromitsu Takahashi^c, Martin Topinka^i, Tomáš Urbanec^g, Jean-Paul Breuer^a, Teruaki Enoto^j, Zsolt Frei^k, Yasushi Fukazawa^c, Gábor Galgóczi^{a,k,l}, Filip Hroch^a, Yuto Ichinohe^m, László L. Kiss^b, Hiroto Matake^c, Tsunefumi Mizuno^c, Kazuhiro Nakazawa^n, Hirokazu Odaka^o, Helen Poon^c, Nagomi Uchida^p, and Yuusuke Uchida^c

aDepartment of Theoretical Physics and Astrophysics, Faculty of Science, Masaryk University, Kotlářská 267/2, Brno 611 37, Czech Republic bKonkoly Observatory, Research Centre for Astronomy and Earth Sciences, Budapest, Hungary cHiroshima University, School of Science, Higashi-Hiroshima, Japan dCzech Aerospace Research Centre, Prague, Czech Republic eSpacemanic Ltd, Bratislava, Slovakia fFaculty of Aeronautics, Technical University of Košice, Slovakia gDepartment of Radio Electronics, Faculty of Electrical Engineering and Communication, Brno University of Technology, Brno, Czech Republic hNeedronix Ltd, Bratislava, Slovakia iINAF - Istituto di Astrofisica Spaziale e Fisica Cosmica, Via A. Corti 12, I-20133 Milano, Italy jThe Hakubi Center for Advanced Research, Kyoto University, Kyoto, Japan kInstitute of Physics, Eötvös Loránd University, Budapest, Hungary lWigner Research Centre, Budapest, Hungary mDepartment of Physics, Rikkyo University, Tokyo, Japan nDepartment of Physics, Nagoya University, Nagoya, Aichi, Japan oDepartment of Physics, The University of Tokyo, Bunkyo-ku, Tokyo, Japan pInstitute of Space and Astronautical Science, Japan Aerospace Exploration Agency, Japan

ABSTRACT We present the detector performance and early science results from GRBAlpha, a 1U CubeSat mission, which is a technological pathfinder to a future constellation of nanosatellites monitoring gamma-ray bursts (GRBs). GRBAlpha was launched in March 2021 and operates on a 550 km altitude sun-synchronous orbit. The gammaray burst detector onboard GRBAlpha consists of a 75×75×5 mm CsI(Tl) scintillator, read out by a dual-channel multi-pixel photon counter (MPPC) setup. It is sensitive in the ∼ 30−900 keV range. The main goal of GRBAlpha is the in-orbit demonstration of the detector concept, verification of the detector’s lifetime, and measurement of the background level on low-Earth orbit, including regions inside the outer Van Allen radiation belt and in the South Atlantic Anomaly. GRBAlpha has already detected five, both long and short, GRBs and two bursts were detected within a time-span of only 8 hours, proving that nanosatellites can be used for routine detection of gamma-ray transients. For one GRB, we were able to obtain a high resolution spectrum and compare it with measurements from the Swift satellite. We find that, due to the variable background, the time fraction of about 67 % of the low-Earth polar orbit is suitable for gamma-ray burst detection. One year after launch, the detector

Further author information: (Send correspondence to J. Řípa) J. Řípa: E-mail: ripa.jakub@gmail.com performance is good and the degradation of the MPPC photon counters remains at an acceptable level. The same detector system, but double in size, was launched in January 2022 on VZLUSAT-2 (3U CubeSat). It performs well and already detected three GRBs and two solar flares. Here, we present early results from this mission as well.

Keywords: gamma-rays; gamma-ray bursts; high-energy astrophysics; nano-satellites; instrumentation; detectors; scintillators; multi-pixel photon counter; low Earth orbit background

1. INTRODUCTION We are living in revolutionary times, when nanosatellites are becoming complementary to large missions and can contribute to our understanding of the high-energy Universe. Several nanosatellite missions and small payloads are being planned, constructed or already launched, e.g. HERMES-TP/SP,^1 GRID,^2 BurstCube,^3 GALI^4 and GTM.^5

The GRBAlpha^{6∗} nanosatellite is a 1U CubeSat which caries an on-board gamma-ray detector capable of detecting hard X-ray / gamma-ray transient sources such as gamma-ray bursts (GRBs).^7 It is a technological pathfinder for a future constellation of nanosatellites CAMELOT^8 monitoring and localizing GRBs using timebased cross-correlation technique.^{9, 10}

The detector onboard GRBAlpha consists of a 75 × 75 × 5 mm CsI(Tl) scintillator read out by eight silicon photomultipliers (SiPM), multi-pixel photon counters (MPPCs) S13360-3050 PE by Hamamatsu, arranged into two independent readout channels with four MPPCs per channel.^{6, 9, 11} The detector is sensitive in the ∼ 30 − 900 keV range with the maximum effective area of ∼ 54 cm^2 at 100 keV.

The satellite was launched from Baikonur by a Soyuz-2.1a rocket to a 550 km altitude Sun-synchronous orbit (SSO) on March 22, 2021. The main goal of GRBAlpha is the in-orbit demonstration of the detector concept, verification of the detector’s lifetime, and measurement of the background level on low-Earth orbit (LEO), including regions inside the outer Van Allen radiation belt and in the South Atlantic Anomaly (SAA).

The main radio ground stations used for commanding the satellite and downloading the scientific data are: the ground station at the Brno University of Technology (Czech Republic); the Bankov ground station run by the Faculty of Aeronautics at the Technical University of Kosice (Slovak Republic) and the ground station at the Piszkéstető observatory (Hungary). The satellite is using amateur radio bands and the housekeeping and scientific data are available via the SatNOGS network^†.

VZLUSAT-2^‡ is a 3U sized CubeSat, developed by the Czech Aerospace Research Centre as a technology mission, with two Earth observing cameras as the primary payload. Among several secondary payloads (X-ray and particle sensors) are two perpendicularly placed GRB detectors. Each detector employs a 75 × 75 × 5 mm CsI(Tl) scintillator read out in the same manner as on GRBAlpha. The detectors are placed under customized solar panels with reduced copper layer for better X-ray transparency.

The satellite was launched from Cape Canaveral (USA) by a Falcon 9 rocket to a 550 km altitude SSO on January 13, 2022. The main radio ground stations used for commanding or downloading the scientific data are: the station of the University of West Bohemia in Pilsen (Czech Republic); the station at the Piszkéstető observatory (Hungary) and the SatNOGS network.

In Sec. 2, we describe the main results of GRBAlpha, in Sec. 3, we present the early results from VZLUSAT-2, and in Sec. 4, we summarize the main conclusions.

2. RESULTS FROM GRBALPHA The GRBAlpha nanosatellite has been successfully operating in orbit for more than one year. Below, we summarize the main results.

∗https://grbalpha.konkoly.hu †https://satnogs.org ‡https://www.vzlusat2.cz/en/

Figure 1. Five gamma-ray bursts (GRB 210807A, GRB 210822A, GRB 210909A, GRB 211018A and GRB 211019A) detected so far by GRBAlpha over-plotted with raw light curves measured by other missions.

2.1 GRB Detections GRBAlpha has so far detected five GRBs, which were simultaneously observed by other satellites. The current version of the onboard payload firmware does not contain a trigger algorithm which would autonomously detect gamma-ray transients because the focus of this mission was mainly to verify the detector concept. The binned count data are recorded on board. The number of spectral bins (up to 256) as well the binning in time is adjustable by a command from ground. Once a new nominal measurement session is started then up to ∼ 8 hours of continuous count rate curves with 4 s temporal resolution and with 4 energy bands are recorded. On ground the GCN^{12§} notices with GRB alerts from Fermi/GBM, Swift/BAT, INTEGRAL/SPI-ACS, AGILE /MCAL, Wind- KONUS, CALET /CGBM, MAXI and other public GRB trigger lists, e.g. ASTROSAT/CZTI GRB archive^¶ and Gamma-ray Urgent Archiver for Novel Opportunities (GUANO)^{13‖} are used to decide which intervals of data recorded by GRBAlpha are worth downloading to search for gamma-ray transients. The five observed GRBs are plotted in Fig. 1.

§https://gcn.gsfc.nasa.gov/gcn_main.html ¶http://astrosat.iucaa.in/czti/?q=grb ‖https://www.swift.psu.edu/guano

The first detection was GRB 210807A (GCN 30624),^{14} which was simultaneously observed by Swift/BAT. This was the first time that a GRB was observed by a 1U CubeSat. It was a long GRB which was detected with a signal-to-noise ratio (SNR) of 8. The data acquisition by GRBAlpha started with 2 × 60 s long exposures and with full spectral resolution of 256 energy channels. Then it was followed by the nominal data acquisition with 4 s temporal resolution in 4 energy bands. By chance the data acquisition with high spectral resolution started when this long GRB was ongoing and therefore we were able to perform a joint spectral analysis with the Swift/BAT data. The spectrum measured by GRBAlpha showed a good agreement with the one measured by Swift/BAT. The best fit power-law has a slope of Γ = 0.90 ± 0.1 and a flux of 1.2 × 10^{−7} erg cm^{−2} s^{−1} in the range of 50 − 300 keV.

The other detected GRBs by GRBAlpha were: long GRB 210822A (GCN 30697)^{15} with SNR≈ 45, short GRB 210909A (GCN 30840)^{16} with SNR=9, long GRB 211018A (GCN 30945)^{17} with SNR=46 and long GRB 211019A (GCN 30946)^{18} with SNR=39.

GRB 210822A has a measured redshift of z=1.736 (GCN 30692),^{19} which for the concordance cosmological model (ΛCDM with H_0 = 69.6 km s^{−1} Mpc^{−1}, Ω_M = 0.29, Ω_0 = 0.71) gives a light travel time of 9.9 Gyr. GRB 211018A and GRB 211019A were detected within only 8 hours, demonstrating that nanosatellites can host payloads sensitive enough to routinely detect GRBs.

Figure 2. The background map at low Earth orbit (530-590 km altitude) as measured by GRBAlpha for E ≳ 110 keV (left) and E ≳ 370 keV (right), respectively. The count rate is averaged in a 2^∘ × 2^∘ pixels grid.

2.2 Low Earth Orbit Background Monitoring The GRBAlpha data also provide valuable information about the background environment at LEO which has several components, e.g. cosmic X-ray background (CXB), cosmic ray particles, geomagnetically trapped particles and albedo (secondary) emission produced in the Earth’s atmosphere.^{20–22} The scintillator based gamma-ray detector is also sensitive to the energetic protons and electrons present in the Van Allen radiation belts (SAA and polar regions).^{23} The advantage of our detector design, which employs MPPC sensors is that it operates at relatively low bias voltage and it can also safely measure inside the extreme radiation conditions of the SAA and polar regions.

GRBAlpha is collecting data to create an average background map at LEO, which will help to estimate the expected duty cycle and to develop the rate trigger algorithms for future GRB missions. For the rate trigger, it is important to know when it should be enabled/disabled in order to avoid an extensive number of false detections. Fig. 2 shows the averaged background maps in two energy bands collected from measurements with temporal resolution of 1, 4, and 15 s.

We noticed an interesting feature in the maps while comparing the measured background levels when the satellite travels from the north southward to the SAA and when it travels northward first passing the SAA. It is displayed in Fig. 3. The measured mean background to the north of the SAA is significantly higher when the satellite passes SAA first. We calculated the mean background for the region of lon = 298^∘-304^∘ and lat = 14^∘-20^∘. The mean count rates are for the northward / southward passes: 105.3 ± 0.7 / 61.2 ± 0.5 (for E ≈ 110 − 370 keV) and 55.9 ± 0.4 / 25.3 ± 0.3 (for E ≈ 370 − 630 keV). This is likely due to the short-term radioactivation background induced by geomagnetically trapped protons in the SAA.^{24–26}

Figure 3. The maps of southward (left panels) and northward (right panels) ground tracks of GRBAlpha, zoomed into the region between the South Atlantic Anomaly (SAA) and the north polar region showing the short-term activation background when the satellite passes SAA and moves northward. The maps show the count rate for the energy band of E ≈ 110 − 370 keV (upper panels) and E ≈ 370 − 630 keV (lower panels). The square in the middle of each panel marks the region in which the average count rate was calculated.

2.3 Long-term Detector Performance One of the objectives of GRBAlpha was to study the aging of S13360-3050 PE MPPCs by Hamamatsu at LEO. As the MPPCs are exposed to geomagnetically trapped protons in the SAA they experience radiation damage which increases dark current and thus noise.^{27} In order to reduce the radiation damage the edge of the detector, where the MPPCs are placed, is shielded by 2.5 mm antimony-lead alloy PbSb4. This shield together with a 1.0 mm Al detector casing provides significant reduction of the total ionizing dose due to geomagnetically trapped and solar protons.^{28} The PbSb4 shield was designed based on the Multi-Layered Shielding Simulation tool (MULASSIS)^{29}

Figure 4. Increase of the low-energy threshold of the detector on board of GRBAlpha plotted from the middle of April 2021 to the middle of May 2022. The shift of the low-energy threshold is caused by the increased noise in MPPCs a result of their gradual degradation due to the irradiation by geomagnetically trapped protons during SAA passages.

Figure 5. An example of the temperature variation measured over four orbits by two thermometers placed on the MPPC board inside the detector casing on GRBAlpha.

implemented in SPENVIS^{∗∗}. Fig. 4 demonstrates the shift of the low-energy threshold over the months since the launch. Before the launch the low-energy threshold was ∼ 10 keV. Three weeks after the launch the threshold was ∼ 29 keV and one year later it was ∼ 56 keV. One year after the launch, the detector performance is good and the degradation of MPPCs remains at an acceptable level.

Fig. 5 shows an example of the temperature variation measured by thermometers placed on the MPPC board of the detector on board of GRBAlpha.

3. RESULTS FROM VZLUSAT-2 The VZLUSAT-2 nanosatellite finished the commissioning phase after the launch and it is now nominally operating. Below are summarized the main results.

3.1 GRB and Solar Flare Detections The GRB payload on VZLUSAT-2 is another technology demonstration and a rate trigger, which would automatically detect GRBs, is not yet implemented in the onboard software. GCN notices and other public GRB trigger lists are used to determine which data sections will be downloaded. There are two GRB detector units on board marked as unit no. 0 and 1. Nominal measurements are done with 1 s temporal resolution in 4 energy bands.

∗∗www.spenvis.oma.be

Figure 6. Three gamma-ray bursts (GRB 220608B, GRB 220423A and GRB220320A) detected so far by the GRB payload on VZLUSAT-2 over-plotted with raw light curves measured by other missions. The bottom panels show the same burst observed by the two perpendicularly placed detector units on VZLUSAT-2.

The GRB payload on VZLUSAT-2 has, at the time of writing, detected three long GRBs: GRB 220320A (GCN 32196)^{30} with SNR=6, GRB 220423A (GCN 31965)^{31} with SNR=28 and GRB 220608B (GCN 31803)^{32} with SNR=46. The events detected by VZLUSAT-2 are plotted in Fig. 6.

The GRB payload on VZLUSAT-2 has also detected two Solar flares which coincide with peaks in the X-ray flux measured by GOES-16 and GOES-17^{††}: on 2022-04-21 (GCN 31937, GCN 31949)^{33, 34} and on 2022-05-20. The observed Solar flares are shown in Fig. 7.

3.2 Low Earth Orbit Background Monitoring Using the GRB payload on VZLUSAT-2, we also construct background maps at LEO. Fig. 8 shows averaged background count rate maps in different energy ranges collected by the detector unit no. 1.

Fig. 9 shows the background variation at low Earth orbit (520-570 km altitude) as measured by the GRB payload (detector unit no. 1) on VZLUSAT-2 for E ≳ 30 keV over about one and half day with 15 s temporal resolution bins. The peaks in the measured background correspond to SAA and polar region passes where the background is dominated by trapped protons and electrons, respectively.

To estimate the fraction of time usable for long GRB detection at a low-Earth SSO, at an altitude of 550 km we consider a median-intensity long GRB (integrated photon flux above 30 keV is 1.19 ph cm^{−2} s^{−1}) based on the Fermi/GBM FERMIGBRST catalog^{‡‡} (for details see Ref.^{21}). Next, using Geant4 Monte Carlo simulations as described in Ref.,^{21} the detector’s effective area of ∼ 50 cm^2 and the best incident angle of a median intensity long GRB, we obtain a detection count rate of 0.58 cnt cm^{−2} s^{−1} for energies E > 30 keV. From this value and from the measured background count rate, we obtain a fraction of time of 67 % usable for the detection of a typical long GRB if the SNR=5 within 15 s integration time is required to claim a detection. Red points in Fig. 9 show the region where a median-intensity long GRB is detectable with the SNR=5.

††https://www.swpc.noaa.gov/products/goes-x-ray-flux ‡‡https://heasarc.gsfc.nasa.gov/W3Browse/fermi/fermigbrst.html

Figure 7. Two solar flares which occurred on 2022-04-21 and on 2022-05-20 detected by the GRB payload on VZLUSAT-2. Top panels show the first solar flare observed by the two perpendicularly placed detector units. The bottom panel shows the second flare over-plotted with the raw light curve measured by Fermi/GBM.

4. SUMMARY The GRBAlpha and VZLUSAT-2 CubeSats are successfully operating at LEO and collecting scientific data. GRBAlpha has so far detected five GRBs, VZLUSAT-2 has so far detected three GRBs and two Solar flares demonstrating that nanosatellites can host payloads sensitive enough to routinely detect gamma-ray bursts. Both satellites are monitoring background at LEO and the maps constructed from these measurements will be useful for the preparation of future GRB missions. The degradation of MPPC sensors on GRBAlpha is being monitored, providing valuable information for future missions which plan to use detectors with MPPC readout. One year after its launch, the GRBAlpha detector performance is good and the degradation of the silicon photon counters remains at an acceptable level.

ACKNOWLEDGMENTS We acknowledge support by the grants KEP2/2020 and SA-40/2021 of the Hungarian Academy of Sciences and Eötvös Loránd Research Network, respectively, for satellite components and payload developments and the grant IF-7/2020 for providing the financial support for ground infrastructure. We acknowledge support by the MUNI Award for Science and Humanities funded by the Grant Agency of Masaryk University and by the European Union’s Horizon 2020 Programme under the AHEAD2020 project (grant agreement n. 871158). This work was supported by JSPS KAKENHI Grant Number 21KK0051, JSPS and HAS under Japan - Hungary Research Cooperative Program, and ISAS/JAXA Grant. We are grateful for the operators and developers of the SatNOGS network, helping us with the reception of the first “sings of life” telemetry messages as well as providing a nice framework for bulk data download from our detectors flying onboard these satellites. We are also grateful to the community of Japanese radio amateurs, including Tetsurou Sato and Masahiro Sanada, who provided support for the GRBAlpha mission.

Figure 8. The background maps at low Earth orbit (520-570 km altitude) as measured by the GRB payload (detector unit no. 1) on VZLUSAT-2 for E ≳ 30 keV (upper left panel), E ≳ 110 keV (upper right panel) and E ≳ 370 keV (bottom panel), respectively. The count rate is averaged in a 2^∘ × 2^∘ pixels grid.

Figure 9. The background variation at low Earth orbit (520-570 km altitude) as measured by the GRB payload (detector unit no. 1) on VZLUSAT-2 for E ≳ 30 keV over about one and half day. The number of counts is in 15 s wide bins. The red points mark the region where a median-intensity long GRB would be detectable with a signal-to-noise ratio SNR=5. This determines the background driven duty cycle.

REFERENCES [1] Fiore, F., Burderi, L., Lavagna, M., Bertacin, R., Evangelista, Y., et al., “The HERMES-technologic and scientific pathfinder,” in [Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series], Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series 11444, 114441R (Dec. 2020).

[2] Wen, J., Long, X., Zheng, X., An, Y., Cai, Z., et al., “GRID: a student project to monitor the transient gamma-ray sky in the multi-messenger astronomy era,” Experimental Astronomy 48, 77–95 (Aug. 2019).

[3] Perkins, J. S., Brewer, I., Briggs, M. S., Bruno, A., Burns, E., et al., “BurstCube: a CubeSat for gravitational wave counterparts,” in [Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series], Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series 11444, 114441X (Dec. 2020).

[4] Rahin, R., Moleri, L., Vdovin, A., Feigenboim, A., Margolin, S., et al., “GALI: a gamma-ray burst localizing instrument,” in [Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series], Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series 11444, 114446E (Dec. 2020).

[5] Chang, H.-K., Lin, C.-H., Tsao, C.-C., Chu, C.-Y., Yang, S.-C., et al., “The Gamma-ray Transients Monitor (GTM) on board Formosat-8B and its GRB detection efficiency,” Advances in Space Research 69, 1249–1255 (Jan. 2022).

[6] Pál, A., Ohno, M., Mészáros, L., Werner, N., Ripa, J., et al., “GRBAlpha: a 1U CubeSat mission for validating timing-based gamma-ray burst localization,” in [Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series], Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series 11444, 114444V (Dec. 2020).

[7] Kouveliotou, C., Wijers, R. A. M. J., and Woosley, S., [Gamma-ray Bursts], Cambridge University Press (2012).

[8] Werner, N., Řípa, J., Pál, A., Ohno, M., Tarcai, N., et al., “CAMELOT: Cubesats Applied for MEasuring and LOcalising Transients mission overview,” in [Space Telescopes and Instrumentation 2018: Ultraviolet to Gamma Ray], den Herder, J.-W. A., Nikzad, S., and Nakazawa, K., eds., Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series 10699, 106992P (July 2018).

[9] Ohno, M., Werner, N., Pál, A., Řípa, J., Galgóczi, G., et al., “CAMELOT: design and performance verification of the detector concept and localization capability,” in [Space Telescopes and Instrumentation 2018: Ultraviolet to Gamma Ray], den Herder, J.-W. A., Nikzad, S., and Nakazawa, K., eds., Society of Photo- Optical Instrumentation Engineers (SPIE) Conference Series 10699, 1069964 (July 2018).

[10] Ohno, M., Werner, N., Pál, A., Mészáros, L., Ichinohe, Y., et al., “The simulation framework of the timingbased localization for future all-sky gamma-ray observations with a fleet of CubeSats,” in [Society of Photo- Optical Instrumentation Engineers (SPIE) Conference Series], Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series 11454, 114541Z (Dec. 2020).

[11] Torigoe, K., Fukazawa, Y., Galgóczi, G., Mizuno, T., Nakazawa, K., et al., “Performance study of a large CsI(Tl) scintillator with an MPPC readout for nanosatellites used to localize gamma-ray bursts,” Nuclear Instruments and Methods in Physics Research A 924, 316–320 (Apr. 2019).

[12] Barthelmy, S. D., Butterworth, P., Cline, T. L., Gehrels, N., Marshall, F., et al., “The GRB coordinates network (GCN): A status report,” in [Gamma-Ray Bursts, 4th Hunstville Symposium], Meegan, C. A., Preece, R. D., and Koshut, T. M., eds., American Institute of Physics Conference Series 428, 99–103 (May 1998).

[13] Tohuvavohu, A., Kennea, J. A., DeLaunay, J., Palmer, D. M., Cenko, S. B., and Barthelmy, S., “Gamma- Ray Urgent Archiver for Novel Opportunities (GUANO): Swift/BAT Event Data Dumps on Demand to Enable Sensitive Subthreshold GRB Searches,” The Astrophysical Journal 900, 35 (Sept. 2020).

[14] Ripa, J., Ohno, M., Takahashi, H., Pal, A., Meszaros, L., et al., “GRB 210807A: Detection by GRBAlpha,” GRB Coordinates Network 30624, 1 (Aug. 2021).

[15] Ohno, M., Ripa, J., Takahashi, H., Pal, A., Meszaros, L., et al., “GRB 210822A: Detection by GRBAlpha,” GRB Coordinates Network 30697, 1 (Aug. 2021).

[16] Ripa, J., Ohno, M., Takahashi, H., Pal, A., Meszaros, L., et al., “GRB 210909A: Detection by GRBAlpha,” GRB Coordinates Network 30840, 1 (Sept. 2021).

[17] Ohno, M., Ripa, J., Takahashi, H., Pal, A., Meszaros, L., et al., “GRB 211018A: Detection by GRBAlpha,” GRB Coordinates Network 30945, 1 (Oct. 2021).

[18] Ripa, J., Ohno, M., Takahashi, H., Pal, A., Meszaros, L., et al., “GRB 211019A: Detection by GRBAlpha,” GRB Coordinates Network 30946, 1 (Oct. 2021).

[19] Zhu, Z. P., Izzo, L., Fu, S. Y., Xu, D., Fynbo, J. P. U., et al., “GRB 210822A: NOT photometry and spectroscopy,” GRB Coordinates Network 30692, 1 (Aug. 2021).

[20] Campana, R., Feroci, M., Del Monte, E., Mineo, T., Lund, N., and Fraser, G. W., “Background simulations for the Large Area Detector onboard LOFT,” Experimental Astronomy 36, 451–477 (Dec. 2013).

[21] Galgóczi, G., Řípa, J., Campana, R., Werner, N., Pál, A., et al., “Simulations of expected signal and background of gamma-ray sources by large field-of-view detectors aboard CubeSats,” Journal of Astronomical Telescopes, Instruments, and Systems 7, 028004 (Apr. 2021).

[22] Campana, R., “In-orbit background for X-ray detectors,” arXiv e-prints 0, arXiv:2205.09359 (May 2022). [23] Řípa, J., Dilillo, G., Campana, R., and Galgóczi, G., “A comparison of trapped particle models in low Earth orbit,” in [Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series], Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series 11444, 114443P (Dec. 2020).

[24] Gruber, D. E., Jung, G. V., and Matteson, J. L., “Radioactivity observed in scintillation counters during the HEAO-1 mission,” in [High-Energy Radiation Background in Space], Rester, A. C., J. and Trombka, J. I., eds., American Institute of Physics Conference Series 186, 232–242 (May 1989).

[25] Odaka, H., Asai, M., Hagino, K., Koi, T., Madejski, G., et al., “Modeling of proton-induced radioactivation background in hard X-ray telescopes: Geant4-based simulation and its demonstration by Hitomi’s measurement in a low Earth orbit,” Nuclear Instruments and Methods in Physics Research A 891, 92–105 (May 2018).

[26] Galgoczi, G., Ripa, J., Dilillo, P., Ohno, M., Campana, R., and Werner, N., “A software toolkit to simulate activation background for high energy detectors onboard satellites,” in [Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series], Society of Photo-Optical Instrumentation Engineers (SPIE) Conference Series 11444, 1144492 (Dec. 2020).

[27] Hirade, N., Takahashi, H., Uchida, N., Ohno, M., Torigoe, K., et al., “Annealing of proton radiation damages in Si-PM at room temperature,” Nuclear Instruments and Methods in Physics Research A 986, 164673 (Jan. 2021).

[28] Řípa, J., Galgóczi, G., Werner, N., Pál, A., Ohno, M., et al., “Estimation of the detected background by the future gamma ray transient mission CAMELOT,” Astronomische Nachrichten 340, 666–673 (Aug. 2019).

[29] Lei, F., Truscott, P. R., Dyer, C. S., Quaghebeur, B., Heynderickx, D., et al., “Mulassis: a geant4-based multilayered shielding simulation tool,” IEEE Transactions on Nuclear Science 49(6), 2788 (2002).

[30] Ripa, J., Pal, A., Ohno, M., Werner, N., Meszaros, L., et al., “GRB 220608B: Detection by VZLUSAT-2,” GRB Coordinates Network 32196, 1 (June 2022).

[31] Ripa, J., Pal, A., Ohno, M., Werner, N., Meszaros, L., et al., “GRB 220423A: Detection by VZLUSAT-2,” GRB Coordinates Network 31965, 1 (Apr. 2022).

[32] Ripa, J., Pal, A., Ohno, M., Werner, N., Meszaros, L., et al., “GRB 220320A: Detection by VZLUSAT-2,” GRB Coordinates Network 31803, 1 (Mar. 2022).

[33] Ripa, J., Pal, A., Ohno, M., Werner, N., Meszaros, L., et al., “GRB 220421B: Detection by VZLUSAT-2,” GRB Coordinates Network 31937, 1 (Apr. 2022).

[34] Ripa, J., Pal, A., Ohno, M., Werner, N., Meszaros, L., et al., “Correction to 31937: GRB 220421B: Detection by VZLUSAT-2,” GRB Coordinates Network 31949, 1 (Apr. 2022).