arXiv:2307.04440v2 [cs.IT] 26 Mar 2024

Time-Frequency-Space Transmit Design and Receiver Processing with Dynamic Subarray for Terahertz Integrated Sensing and Communication

Yongzhi Wu, Graduate Student Member, IEEE, Chong Han, Senior Member, IEEE, and Meixia Tao, Fellow, IEEE

Abstract—Terahertz (THz) integrated sensing and communication (ISAC) enables simultaneous data transmission with Terabitper-second (Tbps) rate and millimeter-level accurate sensing. To realize such a blueprint, ultra-massive antenna arrays with directional beamforming are used to compensate for severe path loss in the THz band. In this paper, the time-frequency-space transmit design is investigated for THz ISAC to generate time-varying scanning sensing beams and stable communication beams. Specifically, with the dynamic array-of-subarray (DAoSA) hybrid beamforming architecture and multi-carrier modulation, two ISAC hybrid precoding algorithms are proposed, namely, a vectorization (VEC) based algorithm that outperforms existing ISAC hybrid precoding methods and a low-complexity sensing codebook assisted (SCA) approach. Meanwhile, coupled with the transmit design, parameter estimation algorithms are proposed to realize high-accuracy sensing, including a wideband DAoSA MUSIC method for angle estimation and a sum-DFT- GSS approach for range and velocity estimation. Numerical results indicate that the proposed algorithms can realize centidegree-level angle estimation accuracy and millimeter-level range estimation accuracy, which are one or two orders of magnitudes better than the methods in the millimeter-wave band. In addition, to overcome the cyclic prefix limitation and Doppler effects, an inter-symbol interference- and inter-carrier interference-tackled sensing algorithm is developed to refine sensing capabilities for THz ISAC.

Index Terms—Terahertz integrated sensing and communications, ultra-massive MIMO, Orthogonal frequency division multiplexing, hybrid beamforming

I. INTRODUCTION A. Background and Motivations

T^{O address the rapidly growing demand for wireless data}

rates and the emergence of new application scenarios, the communication community is seeking new spectrum opportunities as well as new functionalities for sixth-generation (6G) and beyond wireless networks [2]. Following the former trend of moving up to higher frequencies, the Terahertz (THz) band is viewed as one of the key technologies to enable enormous potential in the next-generation advanced transceiver (NGAT) [3]. Another promising usage scenario supported by

This paper was presented in part at IEEE SPAWC, September 2023 [1]. Yongzhi Wu is with the Terahertz Wireless Communications (TWC) Laboratory, Shanghai Jiao Tong University, Shanghai, China (Email: yongzhi.wu@sjtu.edu.cn).

Chong Han is with the Terahertz Wireless Communications (TWC) Laboratory, Department of Electronic Engineering and Cooperative Medianet Innovation Center (CMIC), Shanghai Jiao Tong University, Shanghai, China (Email: chong.han@sjtu.edu.cn).

Meixia Tao is with the Department of Electronic Engineering, Shanghai Jiao Tong University, Shanghai, China (Email: mxtao@sjtu.edu.cn).

the NGAT is integrated sensing and communication (ISAC), which can endow wireless networks with sensing capabilities to realize the mapping of the physical world to the digital world [4]. Leveraging the ultra-broad bandwidth and the ultramassive antenna arrays in the THz band, the integration of these two technologies, i.e., Terahertz integrated sensing and communication (THz ISAC) [5], can achieve ultra-accurate sensing and Terabit-per-second data rates simultaneously.

Despite the promising vision of THz ISAC, critical challenges arise when designing THz ISAC transmit signals. First, there exists severe path loss in the THz band, which includes free path loss, reflection, and scattering losses. These losses strictly limit the maximum sensing and communication distance, and degrade sensing accuracy and data rate. Second, with the power constraints, to compensate for such severe path loss, ultra-massive multiple-input multiple-output (UM- MIMO) antenna arrays with beamforming are used to generate highly directional beams [6]. Thus, energy-efficient and lowcomplexity beamforming algorithms need to be developed. Third, the generation of directional beams restricts the angular coverage of sensing. In general, communication prefers stable beams toward users to enable tractable data detection, while sensing requires sweeping beams to scan possible targets in the surrounding environment [7]. To realize entire-space sensing with directional beams, effective and efficient narrowbeam management schemes, including transmit design in the timefrequency domain and beamforming design in the spatial domain are demanded to realize simultaneous sensing and communication for THz ISAC systems.

Meanwhile, the receive processing encounters significant challenges, especially for sensing parameter estimation algorithms in THz UM-MIMO systems, which are affected by the beamforming architectures and peculiarities of THz channels. First, the sensing algorithm for range and velocity estimation needs to be redesigned, since an additional dimension (namely, spatial domain) is introduced in the received signal model when using the ultra-large dimensional antenna arrays in the THz band. Second, with high channel sparsity due to strong power loss of non-line-of-sight (NLoS) paths, the delay spread of the THz communication channel is reduced [8]. In this case, to utilize broad bandwidth with a fixed subcarrier number, we can increase subcarrier spacing, which is inversely proportional to the symbol duration. Thus, the symbol duration and cyclic prefix (CP) length are reduced in classical multicarrier communication systems, such as orthogonal frequencydivision multiplexing (OFDM). Nevertheless, the round-trip delay of sensing targets should be smaller than the CP duration with classical OFDM sensing algorithms [9]. For communication waveforms with reduced CP, there might exist inter-symbol interference (ISI) effects on the received sensing signal, which cause existing sensing methods inapplicable. Third, as the Doppler shifts are proportional to the carrier frequency, the Doppler effects become even stricter in the THz band. If maintaining current waveform numerology of 5G wireless systems, Doppler effects in the presence of highmobility targets may cause inter-carrier interference (ICI) effects and severely degrade sensing capabilities. Thus, to tackle these challenges, signal processing design in terms of sensing algorithms is vital to realize high-accuracy sensing, while data recovery has been well investigated [10].

B. Related Works

1) Waveform Design: By jointly designing the ISAC transmit signal, sensing and communication can share the hardware and signal processing modules. From the perspective of the time-frequency domain, various ISAC waveforms have been investigated in the literature. As adopted in 4G and 5G standards, CP-OFDM is a promising candidate for ISAC although being a communication-centric design [9], [11]–[15]. Since an OFDM waveform suffers from a high peak-to-average ratio (PAPR) issue, especially in uplink transmission, some singlecarrier waveforms, such as discrete Fourier transform (DFT) spread OFDM (DFT-s-OFDM), are investigated for THz ISAC systems, due to their low PAPR compared to OFDM [16]. Recently, orthogonal time frequency space (OTFS) has been studied in ISAC applications [17]–[19], thanks to its advantages under doubly-selective channels in high-mobility scenarios. Furthermore, a DFT spread OTFS (DFT-s-OTFS) waveform is proposed in [20] to reduce the PAPR of OTFS for THz ISAC. However, the high complexity of data detection for MIMO- OTFS constitutes a serious problem. Despite the PAPR issue, OFDM is still a potential waveform in the THz band, since it has good compatibility with UM-MIMO and enables flexible time-frequency domain resource allocation among multiple users [5]. Thus, wideband UM-MIMO systems with multicarrier modulations are investigated for THz communications in many recent works, including beamforming design [21]– [24], channel estimation [25], multiple access [26], carrier aggregation [27]. Nevertheless, there is a lack of research on THz ISAC in this regard, especially focusing on the transmit design and sensing algorithms in the time-frequency-space domain.

2) Beamforming Design: Pertaining to MIMO-OFDM systems, with conventional fully-digital and analog beamforming architectures, multi-target estimation can be realized by utilizing opportunistic sensing [13] and multibeam optimization [28]. Nevertheless, the fully-digital structure exhibits high hardware complexity and power consumption for THz ISAC systems with large-dimensional antenna arrays, while the analog beamforming architecture can only support one data stream with limited spatial multiplexing gain [6]. As a combined approach, hybrid beamforming can realize comparable data rates with the fully-digital structure and exhibits less hardware complexity. Based on the full-connected (FC) hybrid beamforming architecture, authors in [29] propose a consensus-ADMM approach to design the analog and digital beamformers by jointly optimizing the spectral efficiency (SE) and spatial spectrum matching error of sensing. With the array-of-subarray (AoSA) structure, which further reduces the number of phase shifters and power consumption at the cost of sacrificing data rate, the ISAC hybrid beamformers can be designed by optimizing the Cramér-Rao bound [30] or minimizing the weighted Euclidean distance between the hybrid precoding matrix and the fully digital beamforming matrix [31]. To balance SE and power consumption, a dynamic array-of-subarray (DAoSA) hybrid precoding architecture is proposed in [32], while the ISAC hybrid precoding design with dynamic subarray has not been investigated yet. In addition, most of the aforementioned works design beamformers with some prior knowledge of target angles [13], [29]–[31], [33], which is acceptable in target tracking scenarios but not available in general target estimation, i.e., target discovery mode. Thus, beam scanning-based sensing to discover targets with narrow beams in the THz band is still a significant issue to be addressed.

C. Contributions and Paper Structure

The contributions of this work are summarized as follows: • We present a time-frequency-space transmit design framework for THz ISAC systems by considering a dynamic subarray hybrid beamforming architecture and multi-carrier waveform. In this framework, we develop a vectorization (VEC) based and a sensing codebookassisted (SCA) ISAC hybrid precoding algorithms for the DAoSA structure. Our proposed ISAC hybrid precoding algorithms can realize sensing of the entire angular directions and data transmission by generating scanning sensing beams at different time slots and stable communication beams toward the user. Meanwhile, the proposed VEC algorithm outperforms existing ISAC hybrid precoding methods, and the SCA approach reduces the computational complexity.

• Based on the time-frequency-space domain transmit signal design, we propose parameter estimation algorithms at the sensing receiver, including a wideband DAoSA MU- SIC (W-DAoSA-MUSIC) algorithm for angle estimation, and a sum-DFT and golden section search (S-DFT-GSS) method for range and velocity estimation. Simulation results indicate that the sensing accuracy with the proposed sensing algorithms can achieve centi-degree-level for angle estimation, millimeter-level for range estimation, and decimeter-per-second-level for velocity estimation.

• We further propose an ISI- and ICI-tackled sensing algorithm to overcome the CP limitation on the maximum sensing distance and estimation error caused by highmobility targets. While the ICI is studied in [13], the ISI effects have not been considered in the literature. Compared to the ISI-unaware estimation, the ISI-tackled sensing algorithm can accurately estimate the target with a round-trip delay larger than the CP duration. In contrast

Fig. 1. Based on the DAoSA architecture, the proposed THz ISAC system generates scanning beams toward the q^{th} sensing direction and stable beams toward the communication user at the q^{th} time slot.

with ICI-unaware estimation, the ICI-tackled algorithm can overcome the masking problem of weak targets caused by the side lobes of the strong target in the presence of ICI effects.

The structure of the remainder of this paper is organized as follows. The system framework with the time-frequency-space transmit design for THz ISAC is presented in Sec. II. The ISAC hybrid precoding algorithms are elaborated in Sec. III. The sensing estimation algorithm design with the DAoSA architecture and multi-carrier modulation is proposed in Sec. IV. The ISI- and ICI-tackled sensing algorithm for THz ISAC is developed in Sec. V. Sec. VI illustrates extensive simulation results. Finally, the paper is concluded in Sec. VII.

Notations: C denotes the set of complex numbers; A(i, j) is the entry on the i^{th} row and j^{th} column of A; E{·} defines the expectation operation; The superscripts (·)^T and (·)^H stand for the transpose and Hermitian transpose operations; The notations ⊗ and ⊙ refer to the Kronecker product and Hadamard Product, respectively; det(·) and ‖ · ‖_F denote the determinant and Frobenius norm of a matrix; (·)^† indicates the Moore- Penrose pseudo inverse; vec(·) represents the vectorization operation.

II. SYSTEM FRAMEWORK

As shown in Fig. 1, we propose a THz ISAC system framework based on a wideband UM-MIMO architecture, in which the ISAC transceiver simultaneously senses potential targets in the surrounding spatial environment and sends information symbols to one communication receiver (without loss of generality) via the designed transmit signal in the time-frequency-space domain. Specifically, in the time-frequency domain, the data signal is modulated with orthogonal frequency-division multiplexing (OFDM) and spread across M subcarriers. In the spatial domain, the data streams at each subcarrier are precoded through a digital precoder F_{BB} ∈ C^{N tRF ×Ns} and an analog precoder F_{RF} ∈ C^{Nt ×N tRF} , where N_s denotes the number of data streams and N^t_{RF} refers to the number of transmit RF chains, with N_s ⩽ N^t_{RF} ≪ N_t.

As for the transceiver structure, the ISAC transceiver is equipped with an N_t-element transmit uniform planar array (UPA) to transmit the ISAC waveform and an N_r-element receive UPA to perform sensing echo processing. The communication receiver has an N_r-element UPA to accomplish signal reception and data detection. The transmit antenna arrays adopt a DAoSA hybrid beamforming structure [32]. With the DAoSA structure, the transmit antennas are divided into N^t_{RF} subarrays and each RF chain connects to each subarray with K_t = N_t/N^t_{RF} elements through a switch. Similarly, the received signal is combined through the analog combiner and the digital combiner with N^r_{RF} RF chains, and each receiver subarray contains K_r = N_r/N^r_{RF} elements.

A. Time-Frequency-Space Transmit Design

At the transmitter side, the ISAC system maps the transmitted bit streams to a large amount of data frames. A data frame is divided into Q time slots, each of which contains M × N data symbols, where M and N stand for the numbers of subcarriers and symbols during a time slot. In the multicarrier hybrid beamforming architecture, at the q^{th} time slot, the data symbols s_q [m, n] ∈ C^{Ns ×1}, q = 1, 2, · · · , Q, m = 0, 1, · · · , M − 1, n = 0, 1, · · · , N − 1, which are generated from N_s data streams with E{s_q [m, n]s^H_q [m, n]} =^1_{Ns} I_{Ns} , are first precoded by a digital beamformer F_{BB,q}[m] and mapped to the m^{th} subcarrier in the frequency domain, x_q [m, n] = F_{BB,q}[m]s_q [m, n]. Then, we perform the inverse discrete Fourier transform (IDFT) to transform the frequencydomain data blocks to the time-domain signal and add one cyclic prefix (CP) for each symbol before conducting upconversion and analog beamforming F_{RF,q} ∈ C^{Nt ×N tRF} .

At the q^{th} time slot, the proposed THz ISAC system with the time-frequency-space three-dimensional transmit design generates scanning beams toward the q^{th} sensing direction and stable beams toward the communication user. Note that all subcarriers share the same analog precoder while the digital precoder is performed for each subcarrier [34]. For the n^{th} symbol during the q^{th} time slot, the transmit time-domain signal can be expressed as,

x̃_{q,n}(t) = M−1∑ m=0 F_{RF,q}F_{BB,q}[m]s_q[m, n]e^{j2πmΔf t}, (1)

where t denotes the time instant and Δf refers to the subcarrier spacing. Then, the symbol duration T equals to^1_{Δf} and the total symbol duration is expressed as T_o = T + T_{cp} with the CP duration of T_{cp} =^{Mcp}_M T , where M_{cp} is the CP size. Thus, the duration of a time slot is T_s = NT_o and the frame duration can be expressed as T_f = QT_s. To generate stable beams towards the communication user and scanning beams for searching sensing targets, the transmit beamformers are fixed during a time slot and vary at different time slots.

In this work, we consider a DAoSA hybrid beamforming architecture [32], in which the connections between RF chains and subarrays can be intelligently adjusted through a network of switches. The analog precoding matrix F_{RF,q} can be written as, F_{RF,q} = F_{P,q} ⊙ P_S, (2)

where F_{P,q} ∈ C^{Nt ×N tRF} denotes the phase shifter network matrix and P_S ∈ {0, 1}^{Nt×N tRF} describes the binary switch network matrix, which can be expressed as

P_S = p_{1,1} p_{1,2} . . . p_{1,N} t_{RF} p_{2,1} p_{2,2} . . . p_{2,N} t_{RF} . . . . .. . . . p_N t_{RF,1} p_N t_{RF,2} . . . p_N t_{RF,N} t_{RF}

, (3)

where p_{i,j} stands for the status of the switch between the i^{th} subarray and the j^{th} RF chain. If this switch is closed, p_{i,j} = 1_{Kt} is an all-one vector. Conversely, p_{i,j} = 0_{Kt} is a zero vector. The phase shifter network matrix F_{P,q} satisfies a constant modulus constraint, i.e., the modulus of its elements is 1. Then, the analog precoding matrix F_{RF,q} is given by

F_{RF,q} = f_{1,1} f_{1,2} . . . f_{1,N} t_{RF} f_{2,1} f_{2,2} . . . f_{2,N} t_{RF} . . . . .. . . . f_N t_{RF,1} f_N t_{RF,2} . . . f_N t_{RF,N} t_{RF}

, (4)

where f_{i,j} ∈ C^{Kt ×1} represents the joint precoding vector of the switch and the phase shifters between the i^{th} subarray and the j^{th} RF chain. When this switch is closed, f_{i,j} should satisfy the unit modulus constraint. When the switch is open, f_{i,j} is a zero vector. We denote the feasible set of the analog precoder F_{RF,q} as F. Moreover, the normalized transmit power constraint is expressed as, ‖F_{RF,q}F_{BB,q}[m]‖^2_F = N_s.

B. Communication Model

With multi-carrier transmission, the communication received signal of the m^{th} subcarrier and the n^{th} symbol at q^{th} time slot after the decoding process is expressed as

r_q [m, n] = √ ρC^H_{BB}[m]C^H_{RF}H_c[m]F_{RF,q} F_{BB,q} [m]s_q[m, n] + C^H_{BB}[m]C^H_{RF}n_q [m, n], (5) where ρ describes the average received power, C_{BB}[m] ∈ C^{N rRF ×Ns} is the digital combining matrix, C_{RF} ∈ C^{Nr ×N rRF} is the analog combining matrix, and n_q [m, n] refers to the additive white Gaussian noise with independent and identically distribution CN (0, σ^2_n). In the THz band, the channel is sparse and dominated by the line-of-sight (LoS) path and several reflected rays. Thus, as a benchmark, the multi-path channel model based on ray-tracing methods of the channel matrix H_c[m] at the m^{th} subcarrier can be given by [22], [32], [33],

H_c[m] =γα_L[m]a_r (θ^r_L, ϕ^r_L) a^H_t ( θ^t_L, ϕ^t_L )

+ γ L_N∑

l=1 α_{N,l}[m]a_r ( θ^r_{N,l}, ϕ^r_{N,l} ) a^H_t ( θ^t_{N,l}, ϕ^t_{N,l} ) , (6)

where γ = √_{NtNr} L_N+1 and LN represents the number of non-line-

of-sight (NLoS) paths. Moreover, α_L[m] and α_{N,l}[m] denote the channel gain of the LoS path and l^{th} NLoS path at m^{th} subcarrier, respectively. In addition, θ^r(θ^t) and ϕ^r(ϕ^t) refer to the azimuth and elevation angles of arrival/departure (AoAs/AoDs). In the case of a UPA in the yz-plane with W and L elements on the y and z axes respectively, the array response vector can be expressed by,

a(θ, ϕ) = a_z (ϕ) ⊗ a_y(θ, ϕ), (7)

where

a_y (θ, ϕ) = 1 √ W [1, · · · , e^{jπ(W −1) sin(θ) sin(ϕ)}]^T , (8)

a_z(ϕ) = 1 √ L [1, · · · , e^{jπ(L−1) cos(ϕ)}]^T , (9)

and θ stands for the azimuth angle, and ϕ refers to the elevation angle. When the ratio between the used bandwidth and central frequency is small, the beam squint effect is limited. With the 1024-element UPA at 0.3 THz, the Rayleigh distance is about 1 m, so the near-field effect can be ignored in this paper.

For THz communications, we need to design hybrid precoders to maximize spectral efficiency. The achievable spectral efficiency can be expressed as [32]

R_q = 1 M M−1∑ m=0 log det ( I_{Ns} + ρ N_s R^{−1}_n C^H_{BB}[m]C^H_{RF}H_c[m]

× F_{RF,q}F_{BB,q}[m]F^H_{BB,q}[m]F^H_{RF,q} H^H_c [m]C_{RF}C_{BB}[m] ) , (10)

where R_n = σ^2_nC^H_{BB}[m]C^H_{RF}C_{RF}C_{BB}[m] is a noise covariance matrix. The optimization problem of maximizing R_q at the transmitter side is equivalent to minimizing the Euclidean distance between the optimal fully digital precoder F_c[m] and the hybrid precoder as^1_M ∑_{M−1} m=0 ‖F_c[m]−F_{RF,q} F_{BB,q} [m]‖^2_F .

Generally, the channel state information (CSI) can be known at both transmitter and receiver by utilizing channel estimation [35] and is assumed to be time-invariant during a frame duration. Then, from the singular value decomposition (SVD) of the channel H_c[m], the unconstrained optimal precoder F_c[m] and decoder C_c[m] are comprised of the first N_s columns of the right and the left singular value matrices.

C. Sensing Model

In the THz band, directional beams are used to compensate for severe path loss and improve received sensing signal power, which limits the angular range of sensing targets. To realize entire-space sensing, we design a codebook-based beam-scanning scheme for THz sensing. For the azimuth angle, the whole sensing angular domain is divided into Q scanning directions, ω = [ω_1, ω_2, · · · , ω_Q]^T , each of which corresponds to a time slot. We can set Q = W and design the sensing beamforming vector as the q^{th} column from a discrete Fourier transform (DFT) codebook, by which the transmitter can generate W orthogonal beamforming vectors and steer signals towards W independent sensing directions. Thus, the sensing codebook can be written as,

A = a_z(ϕ) ⊗ [a_{y,1}(ω_1, ϕ), · · · , a_{y,W} (ω_Q, ϕ)] (11)

where

a_{y,q} (ω_q, ϕ) = 1 √ W [1, · · · , e^{jπ(W −1) sin(ωq ) sin(ϕ)}]^T , (12)

and sin(ω_q) = −1 +^1_W + (q − 1)^2_W for q = 1, 2, · · · , W . In this case, the sensing angular window Ω_q at the q^{th} time slot contains angles from arcsin(−1 + (q − 1)^2_W ) to arcsin(−1 + q^2_W ).

At the sensing receiver, the frequency domain received signal of the m^{th} subcarrier and the n^{th} symbol at q^{th} time slot is denoted as y_q [m, n] ∈ C^{N rRF ×1}, which is given by

y_q [m, n] =W^H_{RF,q}H_s[m, n]F_{RF,q} F_{BB,q} [m]s_q[m, n] + W^H_{RF,q} e_q[m, n]

(13)

where W_{RF,q} ∈ C^{Nr ×N rRF} denotes the combing matrix at the sensing receiver and e_q [m, n] represents the AWGN vector. At the ISAC transceiver side, the sensing receiver is collocated with the transmitter. Based on the OFDM radar sensing channel [9], [16] and MIMO channel models [22], [32], the sensing channel matrix H_s[m, n] is expressed as,

H_s[m, n] = √ N_tN_r P P∑ p=1 h_pe^{−j2πmΔf τp} e^{j2π((q−1)Ts +nTo)νp} × a_r(θ_p, ϕ_p)a^T_t (θ_p, ϕ_p), (14)

where P stands for the number of sensing targets, each of which corresponds to one back-reflected path with complex channel coefficient h_p. For the p^{th} target, the delay τ_p and the Doppler shift ν_p are calculated by τ_p =^{2rp}_{c0} (τ_p ⩽ T_{cp}) and ν_p =^{2fc vp}_{c0} (ν_p ≪ Δf), where r_p and v_p refer to the range and relative velocity of the p targets, respectively. c_0 denotes the speed of light and f_c describes the carrier frequency. Moreover, θ_p and ϕ_p represent the azimuth and elevation angle-of-arrival of the p^{th} target.

Beamforming design for sensing aims at achieving the highest beamforming gain towards the sensing direction. Thus, at the q^{th} time slot, the optimal sensing precoder F_{s,q} ∈ C^{Nt ×Ns} can be generated from the q^{th} column of the sensing codebook, namely, F_{s,q} =^{1√}_{Nt} A(:, q)1^T_{Ns} with a normalized factor of 1√ N_t . Then, we need to minimize the Euclidean distance, 1 M ∑_{M−1} m=0 ‖F_{s,q} − F_{RF,q} F_{BB,q} [m]‖^2_F . At the sensing receiver side, W_{RF,q} is fixed during a time slot and the receive sensing beams point to N^r_{RF} random directions within Ω_q at the q^{th} time slot.

D. Problem Formulation

At the THz ISAC transmitter, we need to design the analog and digital beamformers to simultaneously realize a communication link with ultra-fast data rates and provide a desired beampattern for high-accuracy sensing of surrounding targets. Different from the conventional hybrid precoding design problem for communication, the optimal ISAC hybrid precoders should be sufficiently “close” to the time-invariant and frequency-dependent optimal communication precoder and the time-varying and frequency-independent optimal sensing precoder at the same time. Based on the above models and analysis, we can formulate the following multi-objective optimization problem, min F_{RF,q} ,F_{BB,q} [m] { 1 M M−1∑ m=0 ‖F_c[m] − F_{RF,q} F_{BB,q} [m]‖^2_F , 1 M M−1∑ m=0 ‖F_{s,q} − F_{RF,q}F_{BB,q}[m]‖^2_F ] }

s.t. F_{RF,q} ∈ F, ‖F_{RF,q}F_{BB,q}[m]‖^2_F = N_s, m = 0, 1, · · · , M − 1,

(15)

for q = 1, 2, · · · , Q. Since this problem has multiple objective functions and the constraints are non-convex, it is rather difficult to obtain the global optimal solution. In the next section, we propose two algorithms for the THz ISAC hybrid precoding optimization problem to yield near-optimal solutions.

III. HYBRID PRECODING DESIGN FOR THZ ISAC

For the multi-objective ISAC hybrid precoding problem, we can introduce a weighting factor η (0 ≤ η ≤ 1), which provides the tradeoff between sensing and communication. Then, the hybrid precoding problem (15) can be formulated as, min F_{RF,q} ,F_{BB,q} [m] 1 M M−1∑ m=0 ( η‖F_c[m] − F_{RF,q}F_{BB,q}[m]‖^2_F +

(1 − η)‖F_{s,q} − F_{RF,q}F_{BB,q}[m]‖^2_F )

s.t. F_{RF,q} ∈ F, ‖F_{RF,q} F_{BB,q} [m]‖^2_F = N_s, m = 0, 1, · · · , M − 1.

(16)

where η = 0 or η = 1 stands for either sensing-only or communication-only hybrid beamforming design problem. Without loss of generality, we can consider solving the hybrid precoding problem at different time slots separately. Then, a common approach is to use alternating minimization techniques [30], [31], [34], i.e., alternately solving for F_{RF,q} and F_{BB,q}[m]. Hereby, with the irregular structure of the DAoSA analog precoder, we propose an ISAC hybrid precoding algorithm by utilizing the vectorization (VEC) operation in [32].

A. VEC-based ISAC Hybrid Precoding Algorithm

1) Digital Precoding Design: When fixing the analog precoder, we can impose an orthogonal constraint that F_{BB,q}[m] is unitary to mitigate the interference among data streams. Then, the problem (16) can be transferred to, min F_{BB,q} [m] 1 M M−1∑ m=0 ‖G_q [m] − B_q F_{BB,q} [m]‖^2_F

s.t. F_{RF,q} ∈ F, F^H_{BB,q}[m]F_{BB,q}[m] = I_{Ns} , m = 0, 1, · · · , M − 1. (17)

where

G_q [m] = [ √ ηF^T_c [m], √ 1 − ηF^T_{s,q}]^T , (18)

B_q = [ √ ηF^T_{RF,q} , √ 1 − ηF^T_{RF,q}]^T . (19)

Similar to the solution of the so-called Orthogonal Procrustes problem (OPP) [34], the solution to (17) is given by,

F_{BB,q}[m] = V_1U^H , (20)

where G^H_q [m]B_q = UΣV^H is the SVD of G^H_q [m]B_q , and V_1 is the first N_s columns of V.

2) Analog Precoding Design: When fixing the digital precoder, we carry the vectorization process and the analog precoding design problem can be formulated as,

min_{FRF,q} 1 M M−1∑ m=0 ( η‖vec(F_c[m]) − vec(F_{RF,q} F_{BB,q} [m])‖^2+

(1 − η)‖vec(F_{s,q} ) − vec(F_{RF,q}F_{BB,q}[m])‖^2 ) . (21)

After removing the zero elements in vec(F_{RF,q}), we need to solve its non-zero part f_{eff} ∈ C^{Nc Kt×1}, where N_c denotes the number of closed switches. This is a phase rotation problem, whose solution is given by

f_{eff} = exp ( j arg {_{M−1} ∑ m=0 D^H vec ( ηF_c[m]F^H_{BB,q}[m]

+ (1 − η)F_{s,q} F^H_{BB,q}[m] )}) , (22)

where D equals to I_{Nt N} t_{RF} with d_1^{th}, · · · , d_{Nt N} t_{RF−NcKt}^{th} columns punctured, which correspond to the indices of zero elements in vec(F_{RF,q} ). Based on f_{eff}, the effective analog precoder F_{RF,q} can be recovered. With (20) and (22), we can alternatively calculate F_{BB,q} [m] and F_{RF,q} until convergence. After that, we finally update the digital precoders as

F_{BB,q} [m] = √ N_s ‖F_{RF,q}F^†_{RF,q}G_q [m]‖_F

F^†_{RF,q}G_q [m]. (23)

While the VEC algorithm provides a satisfactory solution, it requires a number of iterations in each time slot. Nevertheless, the optimal communication precoder F_c[m] remains the same at different time slots during a frame duration, while only the optimal sensing precoder F_{s,q} changes. Motivated by this, we can calculate the initial solutions of analog and digital precoders from F_c[m] and then update the analog precoders only once at each time slot based on the sensing codebook. Thus, we further propose the following low-complexity sensing codebook-assisted (SCA) ISAC hybrid precoding algorithm.

B. Low-Complexity SCA Algorithm

Instead of using the weighted objective function in (16), we can define a weighted ISAC precoder as, F_q [m] = β( √ ηF_c[m] + √ 1 − ηF_{s,q}) with a normalized factor of β = √ N_s/‖ √ ηF_c[m]+ √ 1 − ηF_{s,q} ‖_F . Before designing the ISAC analog and digital precoders, we can first obtain the solution of analog precoder for the communication-only hybrid precoding design problem,

F_{RF} = arg min

F_{RF},F_{BB}[m] 1 M M−1∑ m=0 ‖F_c[m] − F_{RF}F_{BB}[m]‖^2_F

s.t. F_{RF} ∈ F, ‖F_{RF}F_{BB}[m]‖^2_F = N_s, m = 0, 1, · · · , M − 1, (24)

which can be directly solved by the VEC algorithm.

Based on the initial analog precoder F_{RF}, we can update the analog precoder F_{RF,q} at the q^{th} time slot with the desired sensing beamforming vector A(:, q). Specifically, we calculate the error between the analog precoding vectors of the phase shifters with closed switches and corresponding columns of A(:, q) as,

E_{i,j} =‖A((i − 1)K_t + 1 : iK_t, q) − F_{RF}((i − 1)K_t + 1 : iK_t, j)‖_2,

(25)

for all (i, j) satifying p_{i,j} = 1_{Kt} . Then, we find the first K_s minimum values of E_{i,j} with the indices {(i_1, j_1), · · · , (i_{Ks} , j_{Ks} )}, where K_s = ⌈N_c(1 − η)⌉ denotes the number of subarray beamforming vectors that need to be updated. Next, we can set the designed analog precoder F_{RF,q} = F_{RF} and update it as,

F_{RF,q} ((i_k −1)K_t +1 : i_kK_t, j_k) = A((i_k −1)K_t +1 : i_kK_t, q) (26) for k = 1, · · · , K_s. The digital precoders are calculated as

F_{BB,q} [m] = √ N_s ‖F_{RF,q}F^†_{RF,q} F_q [m]‖_F

F^†_{RF,q} F_q[m]. (27)

IV. SENSING ESTIMATION ALGORITHM DESIGN WITH DAOSA HYBRID BEAMFORMING In this section, we propose the sensing parameter estimation algorithms at the sensing receiver. The task of the sensing receiver is to estimate the angle, range, and velocity of targets, given the transmit signal and the received sensing signal. As the whole sensing angular window is divided into Q scanning directions, at the q^{th} time slot, we only sense the targets whose azimuth angles of arrival are within −Ω_q, given the knowledge of the received signal y_q and the transmit signal s_q .

For angle estimation, multiple signal classification (MUSIC) is a subspace-based method with super-resolution accuracy. Hereby, based on the DAoSA-MUSIC algorithm in [35], we propose the wideband DAoSA-MUSIC algorithm to estimate the target angle by extending to the wideband transmission. We need to reconstruct the observation matrix by performing stacking operations on the received signals at different subcarriers. After estimating each angle parameter, we develop a range and velocity parameter estimation algorithm over two stages, i.e., sum-DFT and golden section search (S-DFT-GSS).

A. W-DAoSA-MUSIC for Angle Estimation

At the q^{th} time slot, we construct the observation vector of the sensing receiver y_q [m, n] ∈ C^{N rRF ×1} as,

y_q [m, n] = W^H_{RF,q}A_rS_q [m, n] + E_q[m, n], (28)

where

S_q [m, n] = Λ_q[m, n]A^T_t F_{RF,q}F_{BB,q}[m]s_q[m, n], (29)

A_r = [a_r(θ_1, ϕ_1), · · · , a_r(θ_P , ϕ_P )], (30)

A_t = [a_t(θ_1, ϕ_1), · · · , a_t(θ_P , ϕ_P )], (31)

Λ_q [m, n] = √ N_tN_r P diag{h^{(q)}_1 [m, n], · · · , h^{(q)}_P [m, n]}, (32)

E_q[m, n] = W^H_{RF,q} e_q[m, n], (33) and h^{(q)}_p [m, n] = h_pe^{−j2πmΔf τp} e^{j2π((q−1)Ts +nTo)νp} . Then, we can stack all y_q [m, n] into one matrix as,

Y_{θ,q} = [ y_{q,0} . . . y_{q,N−1} ] (34)

with y_{q,n} = [y_q [0, n], · · · , y_q [M − 1, n]]. The precoders and the receive steering matrix A_r remain the same at different symbols during a time slot. Then (34) can be written as,

Y_{θ,q} = W^H_{RF,q}A_rS_{θ,q} + E_q , (35)

where S_{θ,q} = [S_q [0, 0], · · · , S_q [M − 1, N − 1]] is regarded as the P ×MN-dimensional equivalent signal source matrix, and E_q ∈ C^{N rRF ×MN} refers to the noise matrix. Based on (35), we can perform the W-DAoSA-MUSIC algorithm to estimate the azimuth AoAs of targets.

Given the reconstructed observation matrix Y_{θ,q}, the covariance matrix can be calculated as,

R_{θ,q} = 1 MN Y_{θ,q}Y^H_{θ,q}. (36)

Then we can conduct the eigenvalue decomposition (EVD) as,

R_{θ,q} = U_sΣ_sU^H_s + U_nΣ_nU^H_n , (37)

where Σ_s ∈ C^{Pq ×Pq} consists of P_q leading eigenvalues, Σ_n ∈ C^{(N rRF −Pq )×(N rRF−Pq )} contains the remaining eigenvalues and P_q denotes the number of targets whose azimuth AoAs are within −Ω_q. With the signal subspace U_s ∈ C^{N rRF ×Pq} and the noise subspace U_n ∈ C^{N rRF ×(N rRF−Pq )}, the pseudo spectrum of W-DAoSA-MUSIC can be formulated as,

P_{music}(θ, ϕ) = a^H (θ, ϕ)W_{RF,q} W^H_{RF,q}a(θ, ϕ) a^H (θ, ϕ)W_{RF,q}U_nU^H_n W^H_{RF,q}a(θ, ϕ)

. (38)

Finally, the AoA estimation (θ̂_p, ϕ̂_p) can be obtained by searching the peaks of the MUSIC spectrum within the angles of −Ω_q, expressed as

(θ̂_p, ϕ̂_p) = arg max_{θ,ϕ} P_{music}(θ, ϕ). (39)

B. S-DFT-GSS for Range and Velocity Estimation For range and velocity estimation, the received signal model can be expressed as,

y_q [m, n] = P∑ p=1 h^{(q)}_p e^{j2πnTo νp} e^{−j2πmΔf τp} x_{p,q}[m, n] + e_q[m, n], (40)

where

x_{p,q} [m, n] = W^H_{RF,q} H_θ(θ_p, ϕ_p)F_{RF,q}F_{BB,q}[m]s_q[m, n], (41)

H_θ(θ, ϕ) = a_r(θ, ϕ)a^T_t (θ, ϕ) (42)

e_q [m, n] = W^H_{RF,q} e_q[m, n] (43)

and h^{(q)}_p = √_{NtNr} P h_pe^{j2π(q−1)Ts νp} . For each estimated AoA parameter (θ̂_p, ϕ̂_p), we can construct a maximum likelihood (ML) estimator by minimizing the log-likelihood function, given by

(τ̂_p, ν̂_p) = arg min_{τ,ν,h}

N^r_{RF}∑

u=1 ‖ ‖ ‖Yu,q − hΨ(τ, ν) ⊙ X̂u,q ‖ ‖ ‖^2_F , (44)

where

Y_{u,q} = y_q (u)[0, 0] . . . y_q (u)[0, N − 1] . . .. . . . y_q (u)[M − 1, 0] . . . y_q (u)[M − 1, N − 1] , (45) Ψ(τ, ν) = Ψ_τ Ψ^T_ν , (46)

X̂_{u,q} = x̂_q (u)[0, 0] . . . x̂_q (u)[0, N − 1] . . .. . . . x̂_q (u)[M − 1, 0] . . . x̂_q (u)[M − 1, N − 1] , (47) with Ψ_τ = [e^{−j2π0Δf τ} , e^{−j2π1Δf τ} , · · · , e^{−j2π(M−1)Δf τ} ]^T , (48) Ψ_ν = [e^{j2π0To ν} , e^{j2π1To ν} , · · · , e^{j2π(N−1)To ν} ]^T , (49) x̂_q [m, n] = W^H_{RF,q} H_θ(θ̂_p, ϕ̂_p)F_{RF,q}F_{BB,q}[m]s_q[m, n], (50)

for u = 1, 2, · · · , N^r_{RF}. Next, this minimization problem can be transformed to the maximization problem,

(τ̂_p, ν̂_p) = arg max_{τ,ν} P_{ML}(τ, ν), (51)

where

P_{ML}(τ, ν) = | | | ∑_N r_{RF}

u=1 Tr (( Ψ(τ, ν) ⊙ X̂_{u,q} )_H Y_{u,q} )| | | 2 ∑_N r_{RF} u=1 ‖Ψ(τ, ν) ⊙ X̂_{u,q}‖^2_F = | | | | | N^r_{RF}∑

u=1 Tr (( Ψ(τ, ν) ⊙ X̂_{u,q} )_H Y_{u,q} ) | | | | | 2

(52)

The solution in (51) is obtained by searching (τ, ν) at which P_{ML}(τ, ν) achieves a maximum value in the region [0,^1_{Δf} ) × [−^1_{2To} ,^1_{2To} ).

To reduce the computational complexity, we can design a two-phase estimation method. Specifically, in the first phase, we operate the on-grid search within a discretized set of delay and Doppler axes with step sizes^1_{MΔf} and^1_{NTo} , which can be implemented with the 2D DFT algorithm. In the second phase, based on the coarse estimation result, we conduct the off-grid estimation by introducing a 2D golden section search (GSS) method. We describe the proposed S-DFT-GSS estimation method in the following.

1) Phase I: To compute the ML estimator in (51), we first perform an on-grid search on the discretized grid Γ = {(^{m0}_{MΔf} ,^{n0}_{NTo} ), m_0 = 0, · · · , M − 1, n_0 = −^N_2 , · · · ,^N_2 − 1}, as (m̂_0, n̂_0) = arg max_{(τ,ν)∈Γ} P_{ML} ( m_0 MΔf , n_0 NT ) . (53)

Hereby, we need to calculate the M × N-dimensional ML estimator profiles on Γ, which can be computed from the sum of N^r_{RF} 2D DFT outputs, given by

P_{ML} ( m_0 MΔf , n_0 NT ) = |g_d (m_0 + 1, [n_0]_N + 1)|^2 (54)

where

g_d =

N^r_{RF}∑

u=1 F^H_M ( X̂^∗_{u,q} ⊙ Y_{u,q} ) F_N , (55)

and F_M ∈ C^{M×M} and F_N ∈ C^{N×N} refer to the normalized DFT matrices. Then we determine that the delay parameter lies between^{m̂0−1}_{MΔf} and^{m̂0 +1}_{MΔf} and the Doppler parameter is between^{n̂0 −1}_{NTo} and^{n̂0+1}_{NTo} . Thus, the search region Γ_g for offgrid estimation in the second phase becomes, { (τ, ν), m̂_0 − 1 MΔf ≤ τ ≤ m̂_0 + 1 MΔf , n̂_0 − 1 NT_o ≤ ν ≤ n̂_0 + 1 NT_o } . (56) 2) Phase II: In this phase, we perform an off-grid search over the continuous-valued region Γ_g , as

(τ̂_p, ν̂_p) = arg max_{(τ,ν)∈Γg} P_{ML}(τ, ν). (57)

Hereby, we can utilize the 2D golden section search technique, each step of which reduces the interval of uncertainty by the golden ratio. Finally, the estimated velocity and range are given by r̂_p =^{τ̂pc0}_2 and v̂_p =^{ν̂pc0}_{2fc} , respectively.

V. ISI- AND ICI-TACKLED SENSING ALGORITHM In the previous section, the proposed estimation algorithm is based on the assumption that the round-trip delay of targets is not longer than the CP duration and the Doppler shifts are much smaller than the subcarrier spacing, i.e., the sensing channel is both ISI- and ICI-free. Nevertheless, when it comes to the THz band, this assumption might become invalid in some cases. First, as the carrier frequency increases, the Doppler shift in the THz band grows much larger than the microwave band, which may cause inter-carrier interference and degrade sensing accuracy, especially in high-mobility scenarios. Second, with the decrease of communication delay spread in the THz band, larger subcarrier spacing can be used and the symbol and CP durations are reduced. However, this limits the maximum sensing distance if still using the proposed ISI- and ICI-unaware sensing algorithm in Sec. IV-B even when the link budget is sufficient.

In this section, we first derive the received signal model with ISI and ICI caused by the sensing channel and then develop an ISI- and ICI-tackled sensing algorithm to overcome the estimation problem with ICI and ISI. Since we take into account the ISI and ICI effects, we focus on the time-frequency domain signal model and design, by simplifying the notations of the spatial domain in this section.

A. Received Signal Model with ICI and ISI

During a time slot, we denote the data signal at the m^{th} subcarrier and the n^{th} symbol as X_{m,n}. Then, the transmit baseband signal with the CP part is expressed as,

s(t) = M−1∑ m=1 N−1∑ n=0 X_{m,n}rect (t − nT_o) e^{j2πmΔf (t−Tcp −nTo)}, (58) where rect(t) refers to a rectangular pulse that is limited to [0, T_o]. At the sensing receiver, the baseband time-domain continuous signal r(t) is given by,

r(t) = P∑ p=1 α_pe^{j2πνpt}s(t − τ_p) + w(t), (59)

where α_p stands for the channel coefficient of the p^{th} target, w(t) denotes the AWGN, delay and Doppler parameters are described in Sec. II-C with relaxing the assumptions τ_p ⩽ T_{cp} into τ_p ⩽ T_s and ν_p ≪ Δf into ν_p < Δf. By sampling the received signal and removing the CP part, we obtain the baseband time-domain discrete signal, r_{m,n} =r(t)|_{t=nTo +Tcp +}^m_{M T} = P∑ p=1 α_pe^{j2πνi (nTo+Tcp + mM T )}s ( nT_o + T_{cp} + m M T − τ_p )

+ w_{m,n}. (60)

Hereby, the key step is to derive the sampling signal s_{τp,m,n} = s ( nT_o + T_{cp} +^m_M T − τ_p ) as M−1∑ m^′=0 N−1∑ n^′ =0

X_m′_{,n}′ rect ( (n − n^′)T_o + T_{cp} + m M T − τ_p )

× e^{j2πm′ Δf} (^{(n−n′)To + mM T −τp}). (61)

When k_pT_o ⩽ τ_p < k_pT_o + T_{cp} with k_p = ⌊^{τi}_{To} ⌋ (⌊·⌋ stands for the floor function), we can obtain

s_{τp,m,n} = M−1∑ m^′=0 X_m′_{,n−kp} e^{j2π m′mM} e^{−j2πm′ Δf τp} e^{j2πm′ kp McpM} . (62)

When k_pT_o + T_{cp} ⩽ τ_p < (k_p + 1)T_o, for m ⩾^{τp}_T M − M_{cp} − k_p(M + M_{cp}), s_{τp,m,n} is the same as that in (62). For m <^τ_T M − M_{cp} − k_p(M + M_{cp}), we obtain s_{τp,m,n} as M−1∑ m^′=0 X_m′_{,n−k−1}e^{j2π m′mM} e^{−j2πm′ Δf τ} e^{j2πm′ k TcpT} e^{j2πm′ McpM} . (63)

Based on the above derivations, we can derive the timedomain input-output relation, i.e., the vector form of the received signal time-domain r_{m,n} at the q time slot, r_q ∈ C^{M N×1} , is expressed as,

r_q = P∑ p=1 α_pΔ^{(νp)}D_N Π^{lp+kpM}_{2MN} vec ( Π^{−lp}_M (D_{lp} Π^{−Mcp}_M + D̂_{lp} )

· F^H_M b_{τp} [X_{q−1}, X_q ] ) + w_q , (64)

where X_q ∈ C^{M ×N} denotes the time-frequency domain transmit signal at the q^{th} time slot, l_p = max{0, ⌈^{τp}_T M −M_{cp}− k_p(M + M_{cp})⌉} (⌈·⌉ describes the ceiling function), Δ^{(νp)} = diag(vec(V_{νp} )) with V_{νp} (m, n) = e^{j2πνp(nTo +Tcp+ mM T )}, the matrix Π_M ∈ C^{M ×M} refers to the forward cyclic-shift (permutation) matrix, D_N equals to the identity matrix I_{2MN} with the first MN rows punctured, D_{lp} equals to the identity matrix I_M with the last M −l_p rows turning into zero elements, D̂_{lp} equals to the identity matrix I_M with the first l_p rows becoming zero elements, b_{τp} = diag{b^0_{τp} , · · · , b^{M−1}_{τp} } with b_{τp} = e^{j2π} ( k_p^{Tcp}_T −^{τp}_T ) , and w_q is the noise vector.

After performing DFT on the matrix form of r_q , R_q = vec^{−1}(r_q ) ∈ C^{M ×N} , we obtain the frequency-domain received signal y_q ∈ C^{M N×1} at the q^{th} time slot, given by

y_q = vec(F_M R_q ) = P∑ p=1 α_pH_p(τ_p, ν_p)[x^T_{q−1}, x^T_q ]^T + w_q ,

(65)

where the matrix H_p(τ_p, ν_p) ∈ C^{MN×2M N} is given by,

H_p(τ_p, ν_p) = (I_N ⊗ F_M )Δ^{(νp)}D_N Π^{lp+kpM}_{2MN} ( I_{2N} ⊗ ( Π^{−lp}_M · (D_{lp} Π^{−Mcp}_M + D̂_{lp} )F^H_M b_{τp} )) , (66)

and x_{q−1} = vec(X_{q−1}), x_q = vec(X_q ). If the ISI and ICI effects are ignored, the input-output relation in the timefrequency domain is approximated as the following matrix form,

Y_q ≈ P∑ p=1 α_pX_q ⊙ Ψ(τ_p, ν_p) + W_q . (67)

The ISI- and ICI-unaware estimation is based on this approximated input-output relation, which is not accurate and causes estimation error in the presence of ISI and ICI effects.

TABLE I SIMULATION PARAMETERS

Notations Definition Value

f_c Carrier frequency 0.3 THz Δf Subcarrier spacing 120 to 3840 kHz T Symbol duration 8.33 to 0.26 μs T_{cp} CP duration^1_4 T M Number of subcarriers {64, 1024} N Number of symbols during a time slot 16 Q Number of time slots during a frame 32 N_t Number of transmit antennas 1024 N_r Number of receive antennas 1024 W Number of antennas on the y-axis 32 L Number of antennas on the z-axis 32 N^t_{RF} Number of transmit RF chains 4 N^r_{RF} Number of receive RF chains 4 N_s Number of data streams 4 N_c Number of closed switches {4, 8, 16}

B. ISI- and ICI-tackled Estimator

Based on the received sensing signal model with ISI and ICI in (65), we can obtain the ISI- and ICI-tackled estimator, given by

(τ̂ , ν̂) = arg max_{τ,ν} ( H_p(τ, ν)[x^T_{q−1}, x^T_q ]^T )_H y_q ‖H_p(τ, ν)[x^T_{q−1}, x^T_q ]^T ‖^2

. (68)

The complexity of the proposed ISI- and ICI-tackled estimation algorithm depends on the computation of H_p(τ, ν)[x^T_{q−1}, x^T_q ]^T . This can be implemented with computationally efficient operations, including FFT algorithms, cyclic shift, vectorization, and Hadamard product. Thus, the overall computational complexity of this estimator is O(MN log(MN)). VI. NUMERICAL RESULTS In this section, we evaluate the sensing and communication performance of the proposed precoding algorithms and sensing parameter estimation methods. The key simulation parameters are listed in Table I, which refer to the physical layer numerology for beyond 52.6 GHz communications in [36] and the THz link budget analysis in [3], [37]. We consider a THz multipath channel with one LoS path and L_N = 4 NLoS paths. In the simulations, we consider 2D beamforming, i.e., all elevation angles are set as ϕ_0 = 90^∘.

A. Performance of Hybrid Precoding Algorithms for THz ISAC

First, we evaluate the performance of the proposed VEC and SCA hybrid precoding algorithms for THz ISAC in terms of spectral efficiency and transmit beamforming gain towards the sensing direction. Specifically, we consider three hybrid precoding architectures, i.e., FC, AoSA, and DAoSA structures. In comparison, the PE-AltMin approach [34] and the TAltMin [31] algorithm are used for the FC and the AoSA structures, respectively. The proposed VEC and SCA algorithms are performed for the DAoSA architecture, which is equivalent to FC with N_c = (N^t_{RF})^2 and AoSA with N_c = N^t_{RF}. Since we focus on the evaluations of the hybrid

Fig. 2. Performance tradeoff between spectral efficiency and transmit sensing beamforming gain when the signal-to-noise ratio (SNR)^ρ_{σ2n} = -20 dB.

Fig. 3. Spectral efficiency versus SNR for the communication link.

precoding design, the FC combining architecture is set at the communication receiver side. Moreover, the performance of fully digital precoding is evaluated as an upper bound. The subcarrier spacing is set as 1.92 MHz and the number of subcarriers equals 64. The signal-to-noise ratio (SNR) of the communication link is -20 dB.

As shown in Fig. 2, the performance tradeoff between spectral efficiency and transmit sensing beamforming gain using different hybrid precoding algorithms is plotted by setting the weighting factor within [0, 1]. We learn that the spectral efficiency decreases as the transmit sensing beamforming gain is improved as expected, since more energy is concentrated toward the sensing direction. In the FC structure, the proposed VEC algorithm performs slightly better than the PE-AltMin approach and achieves close performance to the fully digital precoding. In the AoSA architecture, the VEC algorithm realizes higher spectral efficiency than the TAltMin method when η > 0.5, i.e., communication dominates the precoding design. Moreover, while the proposed VEC algorithm outperforms the SCA method for all dynamic hybrid beamforming structures, the SCA algorithm is more computationally efficient.

Fig. 4. Transmit beampattern in the azimuth plane for η = 0, η = 0.5 and η = 1, when the sensing direction is (−65^∘, 90^∘) and the azimuth angles of communication paths are distributed between −60^∘ and 60^∘.

Next, we investigate the spectral efficiency versus SNR with different numbers of closed switches. In Fig. 3, compared to the communication-only precoding design (η = 1), the spectral efficiency of the ISAC precoding design (η = 0.6) is reduced by approximately 2.5 bits/s/Hz at the SNR of -30 dB. When N_c = 16, the DAoSA structure becomes FC, and the proposed VEC ISAC hybrid precoding algorithm achieves near-optimal performance over the whole SNR range. With fewer closed switches, fewer phase shifters are used, which causes some performance loss while improving energy efficiency.

B. Transmit Beampattern

We illustrate the transmit beampattern of the designed hybrid precoders in Fig. 4 and Fig. 5 for different weights of ISAC precoding design and beam scanning over sequential time slots. As shown in Fig. 4, η = 0 corresponds to the sensing-only precoder F_{s,q}. In this case, both the proposed VEC and SCA can realize the desired beampattern in the FC (N_c = 16) and AoSA (N_c = 4) architectures, which is generated from the DFT sensing codebook. When η becomes 0.5, we learn that the beamforming gain toward the sensing direction is slightly reduced while several communication subbeams are formed and point to the angles of communication paths. In the case of η = 1, the communication-only precoding design does not generate sensing beams toward the sensing direction and concentrates all beams toward the communication receiver. In addition, it is demonstrated that the transmit beam in the FC structure realizes more similar pattern to the fully digital precoding compared with the AoSA structure.

In Fig. 5, it is shown that during a frame duration, the designed THz ISAC transmit signal can generate sweeping beams to scan possible targets in the surrounding environ-

Fig. 5. Beam scanning in the azimuth plane, when the transmit beampattern consists of time-varying sensing beams and stable communications beams. The sensing angular windows are depicted by the shadow areas, which can cover all angles from −90^∘ to 90^∘. In this plot, beam patterns at time slots q = 3, 4, 5, 6 are exhibited.

ment over different time slots and stable beams toward the communication user to enable ultra-fast data transmission. We observe that the transmit beamforming gains toward the sensing direction can achieve approximately 20 dBi as the beam angle varies, while the communication beams remain similar at different time slots.

Complexity Analysis: We denote N_{iter} as the number of iterations of the alternating minimization in the VEC algorithm for each time slot. The overall computational complexity of the VEC-based ISAC hybrid precoding algorithm is given by O(QN_{iter}N^2_t ). Since the SCA ISAC hybrid precoding algorithm does not require the process of alternating minimization for each time slot, it can reduce the computational complexity to O(N_{iter}N^2_t ) compared with the VEC algorithm.

C. Sensing Accuracy

We further investigate the effectiveness of the proposed sensing algorithm with the DAoSA hybrid beamforming architecture. In Fig. 6, a number of sensing targets are randomly distributed between −90^∘ and 90^∘. We conduct beam scanning by using the proposed hybrid precoding algorithms in Sec. III and then plot the normalized range profile based on the back-reflected sensing received signal by using the proposed sensing estimation algorithms in Sec. IV. At the q^{th} time slot, we estimate the parameters of the target within the sensing angular window Ω_q . With the time-frequency-space transmit design, we realize entire-space multi-target sensing, although the directional narrow beams are used in the THz band.

Moreover, we evaluate the sensing accuracy of angle, range, and velocity estimation with the proposed sensing algorithm. In Fig. 7, we set the target parameters including the azimuth angle of 70^∘, the distance of 15 m, and the velocity of 20

(a) (b)

Fig. 6. Angle (degree) and distance (meter) estimation results using the proposed sensing algorithm. (a) Direct plot of the real and estimated values of the target parameters. (b) Normalized angle and range profiles of the estimates.

Fig. 7. Root mean square error (RMSE) for angle, range, and velocity estimation on a target with the azimuth angle of 70^∘, the distance of 15 m, and the velocity of 20 m/s versus the sensing SNR.

m/s. The waveform parameters are M = 64 and Δf = 3.84 MHz. The number of closed switches is 4 at both transmitter and sensing receiver sides. As the sensing SNR increases, the sensing accuracy is improved. Specifically, we observe that the angle, range, and velocity estimation can achieve centidegree-level, millimeter-level, and decimeter-per-second-level accuracy, respectively. In addition, by decreasing the weighting factor η from 0.6 to 0.4, the sensing accuracy is improved, since more power is allocated to the sensing beam.

Complexity Analysis: The computational complexity of EVD in (37) is O((N^r_{RF})^3). Since N^r_{RF} is much smaller than N_r, the overall computational complexity of W-DAoSA- MUSIC mainly depends on the matrix-vector multiplication in (38), namely, O(N^r_{RF}N_r). The computational complexity of the S-DFT-GSS algorithm is O(N^r_{RF}MN log(MN)) in the first phase and O(N_{gss}N^r_{RF}MN) in the second phase, where N_{gss} denotes the iterations of golden section search.

D. ISI and ICI Effects on Sensing Parameter Estimation Finally, we study the ISI and ICI effects on sensing parameter estimation for THz ISAC systems. The subcarrier number is

(a) Three targets have the same velocity v = 5 m/s.

(b) Three targets have the same velocity v = 50 m/s.

Fig. 8. Normalized range profiles of ICI-unaware and -tackled estimations through the sensing channel with weak and strong ICI effects. (a) The scenario contains 3 targets with the ranges (10, 20, 30) m and the effective SNRs (-10, -15, 20) dB considering the beamforming gain. The waveform parameters are M = 1024 and Δf = 120 kHz.

set as 1024. The considered scenario contains 3 targets with the ranges (10, 20, 30) m and the effective SNRs (-10, -15, 20) dB considering the beamforming gain. In Fig. 8, we compare the ICI-unaware and ICI-tackled estimation algorithms under two cases, i.e., sensing channels with weak and strong ICI effects, respectively. As shown in Fig. 8(a), the velocity of targets is set as 5 m/s, which corresponds to the low-mobility scenario. In this case, we learn that both ICI-unaware and ICI-tackled sensing algorithms have similar estimation results and can accurately estimate the parameters of 3 targets. Nevertheless, when the target velocity increases to 50 m/s in Fig. 8(b), with ICI-unaware estimation, ICI effects increase side-lobe levels of the target with the strongest power, which may cause masking of weak targets or large errors on the parameters of the other two targets. The distance of the target at 30 m is estimated as 29.4 m and the target at 20 m cannot be detected successfully due to the ambiguity caused by side lobes. In contrast, the proposed ICI-tackled sensing algorithm can overcome this problem and still accurately estimate these three targets.

In Fig. 9, we consider the ISI effects on THz ISAC systems.

(a) Δf = 480 kHz, the CP-limited maximum sensing distance is 78 m, and the sensing channel is ISI-free.

(b) Δf = 3840 kHz, the CP-limited maximum sensing distance is 9.8 m, and there exist ISI effects.

Fig. 9. Normalized range profiles of ISI-unaware and -tackled estimations through the sensing channel without and with ISI effects. (a) The scenario contains 2 targets with the ranges (10, 45) m, the same velocity v = 5 m/s, and the effective SNRs (-10, -10) dB considering the beamforming gain. The subcarrier number is M = 1024.

We consider the scenario containing 2 targets with the ranges (10, 45) m, the same velocity v = 5 m/s, and the effective SNRs (-10, -10) dB considering the beamforming gain. As shown in Fig. 9(a), when the subcarrier spacing is 480 kHz, the CP-limited maximum sensing distance is 78 m, which is longer than the target ranges. In this case, there is no ISI effect and we can obtain accurate estimated values of target ranges by using the ISI-unaware sensing algorithm. When the delay spread of the THz communication channel decreases, we can increase the subcarrier spacing and the CP duration becomes shorter, which reduces the CP-limited sensing distance. In Fig. 9(b), the subcarrier spacing increases to 3.84 MHz, and the CP-limited sensing distance is 9.8 m, which is shorter than the target ranges. Thus, there exist ISI effects on the received sensing signal. According to the normalized range profile using the ISI-unaware sensing algorithm, the range of the second target is estimated as 49 m, while the ground truth is 45 m. By comparison, the ISI-tackled sensing algorithm still performs well and is robust against the ISI effect.

VII. CONCLUSION In this paper, we have proposed a THz ISAC system framework, including the time-frequency-space transmit design with the DAoSA hybrid beamforming architecture and OFDM waveform, and sensing algorithms for angle, range, and velocity estimation. We propose two ISAC hybrid precoding algorithms, i.e., the near-optimal VEC method and the low-complexity SCA approach. Meanwhile, in the ISIand ICI-free case, we propose the W-DAoSA-MUSIC angle estimation algorithm and the S-DFT-GSS range and velocity estimation method. Furthermore, when there exist ISI and ICI effects on target estimation in the THz band, we develop the ISI- and ICI-tackled sensing algorithm to overcome the CP limitation and high-mobility target estimation problem.

With extensive simulations, the results indicate that the proposed VEC ISAC hybrid precoding algorithm can achieve close performance to fully digital precoding and outperforms other existing methods. The developed SCA algorithm can reduce computational complexity by removing the process of alternating minimization for each time slot. Meanwhile, with the proposed estimation algorithms, centi-degree-level angle estimation, millimeter-level range estimation, and decimeterper-second-level velocity estimation can be realized in THz ISAC systems. Moreover, an implementation demo of OFDM waveform based THz communication system can be found in our video https://twclabsjtu.github.io/THz-ISAC-System/.

REFERENCES

[1] Y. Wu and C. Han, “Time-frequency-space signal design with dynamic subarray for terahertz integrated sensing and communication,” in Proc. of IEEE International Workshop on Signal Processing Advances in Wireless Communications (SPAWC), 2023.

[2] W. Tong and P. Zhu, “6G: The Next Horizon: From connected people and things to connected intelligence,” Cambridge University Press, 2021.

[3] I. F. Akyildiz et al., “Terahertz band communication: An old problem revisited and research directions for the next decade,” IEEE Transactions on Communications, vol. 70, no. 6, pp. 4250–4285, 2022.

[4] F. Liu et al., “Integrated sensing and communications: Toward dualfunctional wireless networks for 6G and beyond,” IEEE Journal on Selected Areas in Communications, vol. 40, no. 6, pp. 1728–1767, 2022.

[5] C. Han et al., “THz ISAC: A physical-layer perspective of terahertz integrated sensing and communication,” IEEE Communications Magazine, vol. 62, no. 2, pp. 102–108, 2024.

[6] C. Han et al., “Hybrid beamforming for terahertz wireless communications: Challenges, architectures, and open problems,” IEEE Wireless Communications, vol. 28, no. 4, pp. 198–204, 2021.

[7] J. A. Zhang et al., “Enabling joint communication and radar sensing in mobile networks—a survey,” IEEE Communications Surveys & Tutorials, vol. 24, no. 1, pp. 306–345, 2022.

[8] C. Han et al., “Terahertz wireless channels: A holistic survey on measurement, modeling, and analysis,” IEEE Communications Surveys & Tutorials, vol. 24, no. 3, pp. 1670–1707, 2022.

[9] C. Sturm and W. Wiesbeck, “Waveform design and signal processing aspects for fusion of wireless communications and radar sensing,” Proceedings of the IEEE, vol. 99, no. 7, pp. 1236–1259, 2011.

[10] H. Sarieddeen et al., “An overview of signal processing techniques for terahertz communications,” Proceedings of the IEEE, vol. 109, no. 10, pp. 1628–1665, 2021.

[11] C. R. Berger et al., “Signal processing for passive radar using OFDM waveforms,” IEEE Journal of Selected Topics in Signal Processing, vol. 4, no. 1, pp. 226–238, 2010.

[12] J. Johnston et al., “MIMO OFDM dual-function radar-communication under error rate and beampattern constraints,” IEEE Journal on Selected Areas in Communications, vol. 40, no. 6, pp. 1951–1964, 2022.

[13] M. F. Keskin et al., “MIMO-OFDM joint radar-communications: Is ICI friend or foe?” IEEE Journal of Selected Topics in Signal Processing, vol. 15, no. 6, pp. 1393–1408, 2021.

[14] J. A. Zhang et al., “Multibeam for joint communication and radar sensing using steerable analog antenna arrays,” IEEE Transactions on Vehicular Technology, vol. 68, no. 1, pp. 671–685, 2019.

[15] K. Wu et al., “Integrating low-complexity and flexible sensing into communication systems,” IEEE Journal on Selected Areas in Communications, vol. 40, no. 6, pp. 1873–1889, 2022.

[16] Y. Wu et al., “Sensing integrated DFT-spread OFDM waveform and deep learning-powered receiver design for terahertz integrated sensing and communication systems,” IEEE Transactions on Communications, vol. 71, no. 1, pp. 595–610, 2023.

[17] L. Gaudio et al., “On the effectiveness of OTFS for joint radar parameter estimation and communication,” IEEE Transactions on Wireless Communications, vol. 19, no. 9, pp. 5951–5965, 2020.

[18] S. K. Dehkordi et al., “Beam-space MIMO radar for joint communication and sensing with OTFS modulation,” IEEE Transactions on Wireless Communications, pp. 1–1, 2023.

[19] K. Wu et al., “OTFS-based joint communication and sensing for future industrial IoT,” IEEE Internet of Things Journal, vol. 10, no. 3, pp. 1973–1989, 2023.

[20] Y. Wu et al., “DFT-spread orthogonal time frequency space system with superimposed pilots for terahertz integrated sensing and communication,” IEEE Transactions on Wireless Communications, 2023.

[21] H. Yuan et al., “Hybrid beamforming for mimo-ofdm terahertz wireless systems over frequency selective channels,” in Proc. of IEEE Global Communications Conference (GLOBECOM), 2018.

[22] H. Yuan et al., “Hybrid beamforming for terahertz multi-carrier systems over frequency selective fading,” IEEE Transactions on Communications, vol. 68, no. 10, pp. 6186–6199, 2020.

[23] L. Yan et al., “Energy-efficient dynamic-subarray with fixed true-time-delay design for terahertz wideband hybrid beamforming,” IEEE Journal on Selected Areas in Communications, vol. 40, no. 10, pp. 2840–2854, 2022.

[24] F. Gao et al., “Wideband beamforming for hybrid massive MIMO terahertz communications,” IEEE Journal on Selected Areas in Communications, vol. 39, no. 6, pp. 1725–1740, 2021.

[25] K. Dovelos et al., “Channel estimation and hybrid combining for wideband terahertz massive mimo systems,” IEEE Journal on Selected Areas in Communications, vol. 39, no. 6, pp. 1604–1620, 2021.

[26] B. Zhai et al., “SS-OFDMA: Spatial-spread orthogonal frequency division multiple access for terahertz networks,” IEEE Journal on Selected Areas in Communications, vol. 39, no. 6, pp. 1678–1692, 2021.

[27] L. Samara et al., “Adapt and aggregate: Adaptive OFDM numerology and carrier aggregation for high data rate terahertz communications,” IEEE Journal of Selected Topics in Signal Processing, 2023.

[28] Y. Luo et al., “Optimization and quantization of multibeam beamforming vector for joint communication and radio sensing,” IEEE Transactions on Communications, vol. 67, no. 9, pp. 6468–6482, 2019.

[29] Z. Cheng et al., “Hybrid beamforming design for OFDM dual-function radar-communication system,” IEEE Journal of Selected Topics in Signal Processing, vol. 15, no. 6, pp. 1455–1467, 2021.

[30] X. Wang et al., “Partially-connected hybrid beamforming design for integrated sensing and communication systems,” IEEE Transactions on Communications, vol. 70, no. 10, pp. 6648–6660, 2022.

[31] F. Liu and C. Masouros, “Hybrid beamforming with sub-arrayed MIMO radar: Enabling joint sensing and communication at mmWave band,” in Proc. of IEEE International Conference on Acoustics, Speech and Signal Processing (ICASSP), 2019.

[32] L. Yan et al., “A dynamic array-of-subarrays architecture and hybrid precoding algorithms for terahertz wireless communications,” IEEE Journal on Selected Areas in Communications, vol. 38, no. 9, pp. 2041– 2056, 2020.

[33] A. M. Elbir et al., “Terahertz-band joint ultra-massive MIMO radarcommunications: Model-based and model-free hybrid beamforming,” IEEE Journal of Selected Topics in Signal Processing, vol. 15, no. 6, pp. 1468–1483, 2021.

[34] X. Yu et al., “Alternating minimization algorithms for hybrid precoding in millimeter wave MIMO systems,” IEEE Journal of Selected Topics in Signal Processing, vol. 10, no. 3, pp. 485–500, 2016.

[35] Y. Chen et al., “Millidegree-level direction-of-arrival estimation and tracking for terahertz ultra-massive mimo systems,” IEEE Transactions on Wireless Communications, vol. 21, no. 2, pp. 869–883, 2022.

[36] T. Levanen et al., “Mobile communications beyond 52.6 GHz: Waveforms, numerology, and phase noise challenge,” IEEE Wireless Communications, vol. 28, no. 1, pp. 128–135, 2021.

[37] K. Rikkinen et al., “THz radio communication: Link budget analysis toward 6G,” IEEE Communications Magazine, vol. 58, no. 11, pp. 22– 27, 2020.