arXiv:1601.01249v4 [physics.ins-det] 7 Jul 2016

Simulations of background sources in AMoRE-I experiment

A. Luqman^a, D.H. Ha^a, J.J. Lee^b, E.J. Jeon^{c,∗}, H.S. Jo^c, H.J. Kim^a, Y.D. Kim^c, Y.H. Kim^{c,d}, V.V. Kobychev^e, H.S. Lee^c, H.K. Park^c, K. Siyeon^b, J.H. So^c, V.I. Tretyak^e, Y.S. Yoon^{c,∗}

aDepartment of Physics, Kyungpook National University, DaeGu 41566, Korea bDepartment of Physics, Chung-Ang University, Seoul 06974, Korea cCenter for Underground Physics, Institute for Basic Science, Daejeon 34047, Korea dKorea Research Institute of Standards and Science, Daejeon 34113, Korea eInstitute for Nuclear Research, MSP 03680 Kyiv, Ukraine

Abstract The first phase of the Advanced Mo-based Rare Process Experiment (AMoRE- I), an experimental search for neutrinoless double beta decay (0νββ) of^{100}Mo in calcium molybdate (^{40}Ca^{100}MoO_4) crystal using cryogenic detection techniques, is in preparation at the YangYang underground laboratory (Y2L) in Korea. A GEANT4 based Monte Carlo simulation was performed for the first-phase AMoRE detector and shield configuration. Background sources such as^{238}U, 232Th,^{235}U, and^{210}Pb from inside the crystals, surrounding materials, outer shielding walls of the Y2L cavity were simulated. The estimated background rate in the region of interest was estimated to be <1.5 ×10^{−3} counts/keV/kg/yr (ckky). The effects of random coincidences between backgrounds and twoneutrino double beta decays of^{100}Mo as a potential background source were estimated to be <2.3 ×10^{−4} ckky.

Keywords: Background simulation, detectors, neutrinoless double beta decay, underground experiment

∗Corresponding authors Email addresses: ejjeon@ibs.re.kr (E.J. Jeon), ysy@ibs.re.kr (Y.S. Yoon)

Preprint submitted to Journal of L^ATEX Templates February 8, 2018

1. Introduction

As of today, on the basis of results from a number of neutrino oscillation experiments, it is known that neutrinos have mass. However, their absolute mass scale is still not known [1, 2, 3]. The half-life of neutrinoless double beta decay (0νββ) of certain nuclei is related to the effective Majorana neutrino mass, and 5 the investigation of neutrinoless double beta decays is the only practical way to determine the absolute neutrino mass scale and the nature of the neutrino such as Majorana or Dirac particle [3]. The Advanced Mo-based Rare Process Experiment (AMoRE) [4] is an experimental search for neutrinoless double beta decays of^{100}Mo nuclei using^{40}Ca^{100}MoO_4 (CMO) scintillating crystals operat- 10 ing at milli-Kelvin temperatures and being planned to operate at the YangYang underground laboratory (Y2L) in Korea. The AMoRE experiment will run in a series of phases [5]; the first phase of the experiment (AMoRE-I) will use a ∼5 kg (possibly, up to 10 kg) array of CMO crystals. The goal of background level for AMoRE-I is 0.002 counts/keV/kg/yr (ckky) in the region of interest (ROI), 15 3.034 ± 0.01 MeV. Radiations originating from the CMO crystals themselves are known to be the dominant source of backgrounds [6]. Other possible sources are activities from radioisotopes contained in the^{238}U,^{232}Th, and^{235}U decay chains from materials in the nearby detector system and the outer lead shielding box that produce signals in the crystals. Backgrounds from more remote 20 external sources such as the surrounding rock material and cement floor are also considered as possible sources. Random coincidences of radiations from different background sources with two-neutrino double beta (2νββ) decays of^{100}Mo in the CMO is known as a possible background source in the ROI [7, 8]. In this paper we estimate background rates due to the above mentioned background 25 sources by performing simulations.

2. The AMoRE-I Experiment

2.1. The geometry for detector simulation

The detector geometry used for the AMoRE-I simulation includes thrity-five CMO crystals, shielding layers internal to the cryostat, an external lead shielding 30 box, and outer rock walls of the Y2L cavity. Each crystal has a cylindrical shape with 4.5 cm diameter, 4.5 cm height, and mass of 310 g. The total mass of crystals is 10.9 kg, originated from initial design of AMoRE-I experiment. The thirty-five crystals are arranged in seven columns, each with five crystals stacked coaxially, with the center column surrounded by six external ones. The side, 35 bottom and portion of top surfaces of each crystal are covered by a 65 μm-thick Vikuiti Enhanced Specular Reflector film (former VM2000) [9]. Each crystal is mounted in a copper frame, which is a complicated design in reality, but, in the simulation, a simplified CMO supporting copper frame with corresponding mass is used, as shown in Fig. 1. A Ge wafer and its copper frame are located above 40 each crystal and below the lowest crystal. More detailed detector description can be found elsewhere [5, 10].

The whole crystal assembly is enclosed in a cylindrical 2-mm-thick lead superconducting magnetic shielding tube (diameter of 40.0 cm and height of 44 cm) with top and bottom discs, which is made of an ultra-low activity, ancient 45 lead, as shown in Fig. 2. A 1-cm-thick copper plate and 10-cm-thick lead plate (diameter of 40.8 cm and mass of 148.3 kg) are located in series above the CMO crystal assembly, to attenuate backgrounds from materials above crystals inside the cryostat, such as wires, temperature sensors, heaters, G10 fiberglass tubes, and stainless steel tubes. The crystal assembly is placed inside of four concen- 50 tric copper cylinders with total Cu thickness of 10 mm, all within a 5 mm-thick outer stainless-steel vacuum cylinder, as shown in Fig. 2. Top plates of shields are connected with G10 fiberglass tubes, which are made of a woven fiberglass material with 12 cm-height, 2.5 cm-diameter (∼25 g) and are known as a material with high radioactive background. In this simulation, simple top plates and 55 G10 fiberglass tubes are taken into account in the detector geometry. Realistic

(a) (b) (c)

Figure 1: (a) A CMO crystal (yellow) with Vikuiti reflector (light green) and CMO supporting copper frame (brown). Top of the reflector is open for a Ge wafer. (b) Vikuiti reflector surrounding each crystal except for the center area on the top. (c) 35 CMO crystals are stacked in 5 layers and 7 columns.

structures and features will be included on top plates in future simulations.

The cryostat is located inside a 15-cm-thick external lead shield, a total mass of ∼15.6 ton. A top lead shield plate, covering area of 150×150 cm^2, is placed ∼50-cm above the top of the cryostat gives a space for pipes and 60 valves of the cryostat in the detector system. For radiations from the rock walls surrounding the experimental enclosure, the simulation uses a 50-cm-thick spherical rock shell, which is an optimized thickness for saturated escaping γrays. For radiations from the laboratory environment such as the cement floor, the laboratory walls and ceiling, and iron supporting system, simplified designs 65 are implemented into the geometry as shown in Fig. 3.

2.2. Simulation method

We have performed simulations using the GEANT4 Toolkit [11]. In internal or external materials, radioactive sources such as full decay chains of^{238}U, 232Th, and^{235}U are simulated. In general, most decay sources and their daugh- 70 ters are considered to be in equilibrium states, thus all related activities within

(a) (b)

Figure 2: Outside the cryostat, a 15 cm-thick outer lead shield is located. The cryostat is composed of a stainless steel shield and four Cu shields. Top plates of cryostat shields are connected with G10 fiberglass tubes (a). All the way inside the cryostat, an inner lead plate (gray) on a top of a Cu plate is located above crystals. A 2-mm-thick superconducting lead shield surrounds crystals inside the cryostat.

the chains are simply equal to^{238}U,^{232}Th, and^{235}U activities multiplied by the branching ratios for decays of the daughter isotopes. However, for^{238}U decays inside crystals, a broken decay chain is considered by measured^{238}U and 222Rn concentrations separately. For radiations from rock, instead of^{40}K and 75 full decay chain simulation of^{238}U and^{232}Th nuclei, γs with energy of 1.46, 1.87, and 2.61 MeV, are simulated at the rock shell, since daughter nuclei, α, and β cannot penetrate the lead shield and the cryostat, made of stainless steel and copper shields.

Each simulated event includes deposits inside crystals within an event win- 80 dow of 100 ms when a decay occurs, which is based on a few times of a typical

Figure 3: Cement floor, laboratory walls, ceiling of Y2L laboratory. The ceiling and walls are covered by plaster board and steel plate in series.

pulse width (∼20-30 ms) in cryogenic measurements [10]. Sometimes decays with relatively short half lifetime such as^{212}Po decay with a half lifetime of 300 ns and the followed decays will appear in the same event, called pileup events, and they were treated as one event in simulated event. Furthermore, effect of 85 random coincidence of^{100}Mo 2νββ decay events and other radioactive sources inside crystals were estimated by a convolution technique. For random coincidence rate calculation,^{100}Mo 2νββ decay events were generated using an event generator, DECAY0 program [12], and those events were used as input particles in our simulation package with the AMoRE-I detector configuration to get a 90 distribution of^{100}Mo 2νββ decays inside the CMO crystals.

3. Analysis

Radioactive sources are simulated in the following materials which are known as dominant background sources: (i) First, the internal background in CMO crystals (ii) Second, backgrounds from materials in the detector system, in- 95 cluding CMO supporting copper frame, Vikuiti reflector, superconducting lead shield, Cu plate under internal lead, internal lead plate, G10 fiberglass tubes, and outer lead shielding box (iii) Third, backgrounds from rock material and surrounding underground laboratory. Then, we estimate an anti-coincidence rate and a random coincidence rate with the^{100}Mo 2νββ decays. 100 Anti-coincidence rate is estimated from events in the ROI in one crystal, called a single hit event, while events with hits in more than one crystal are rejected because they are obviously from radioactive decays. The single hit events are surface α events, β-α pileup events, and β-like (β or γ) events. First, the surface α-events from crystals or near-by materials can deposit energies in 105 the crystals in a continuum distribution up to Q-value (see Section 3.2.1 and Ref. [13]), which can appear in the ROI. Those α signals are distinguished from β and γ signals by a pulse shape discrimination (PSD) and a separation power of 7.6 σ between α and β/γ events were reported [14]. We assume that the α event rejection power is 99.9999 % in this estimation. Second, the β-α pileup 110 events are from decays of (^{212}Bi+^{212}Po) in^{232}Th decay chain, with half lifetime of 300 ns, and decays of (^{214}Bi+^{214}Po) in^{238}U decay chain, with half lifetime of 164 μs. When the β-α pileup events occur near the surface of crystals or near-by materials, events with a faction of α Q-value and β-energy can appear in the ROI. These β-α pileup events from^{238}U and^{232}Th chains can be rejected 115 by the PSD analysis with a rejection power of 99 %, which was reported with a clear separation between α and β-like events with a prototype detector [14, 5]. In this estimation, 90 % rejection efficiency (∼1.6 σ) is assumed, conservatively. After the surface α rejection, remaining anti-coincidence rate is mainly β-like single hit event rate in the ROI. A further rejection scheme for β-like single hit 120 events will be discussed in Section 3.1.1.

Random coincidence events are originated from any two signals, while the β-α pileup events are from two consecutive decays with relatively short half lifetimes. When two random signals occurred within a time resolution, they might be considered as one pulse, which could be a background source in the ROI. Ran- 125 dom coincidence event rate within a time resolution of 0.5 ms were estimated by a convolution of two background spectra [15]. The Random coincidence rate includes not only randomly coincident events by two^{100}Mo 2νββ decays, but those by a^{100}Mo 2νββ decay and another decays from other background sources

(see Section 3.1.2). 130 Activities of^{238}U,^{232}Th, and^{235}U which are used to normalize the simulation results, were measured by a germanium counting and inductively coupled plasma mass-spectroscopy (ICP-MS). The High Purity Germanium (HPGe) measurements were performed at the Y2L [16]. The ICP-MS measurements were all performed by the KAIST Analysis Center for Research Advancement 135 (KARA), Korea. The activity of backgrounds in a CMO crystal was measured by low temperature detector technique [14]. Activities of some materials were from published references. The concentration of materials are listed in the following section. Here, the activities from bulk and surface contaminations are considered as uniform for crystals and near-by materials. The surface alpha 140 events are also from external contaminations [17], which will be studied in the future.

3.1. Internal background in CMO crystals 3.1.1. Background rate due to sources inside CMO crystals

The activities inside crystals, listed in Table 1, are from a recent measure- 145 ment of a CMO crystal [18], except the activity of^{232}Th. For the activity of^{232}Th, a conservative upper limit are used. Using activities of radioactive sources in crystals, event rates in the ROI are normalized to the unit of counts/keV/kg/yr (ckky). Fig. 4 shows deposited energy distributions in CMO crystals for total single-hit event rate, β-α pileup rate, and β-like event rate 150 exclusively.

Table 1: Activities based on a CMO crystal measurement [18] [mBq/kg]

210Pb^{238}U^{226}Ra(^{222}Rn)^{232}Th^{235}U(^{211}Bi) Activity 7.3 0.98 0.065 <0.05 0.47

As shown in Fig. 4, β-like events from^{208}Tl decay in^{232}Th chain is a dominant source candidate in the ROI, but they can be rejected using a time correlation with the α signal from the preceding^{212}Bi→^{208}Tl α decay, called α-tagging method. Rejection of all events occurring within 30 mins after an 155 α event with 6.207 MeV in the same crystal, results in a 97.4% veto efficiency for^{208}Tl-induced β events in the^{100}Mo 2νββ signal region, while introducing ∼1% dead-time.

Figure 4: Single hit event rate distribution from (a)^{238}U and (b)^{232}Th inside crystals for total events(red) including αs, β-α pileup events (pink), and β-like event exclusively (blue). The difference between the total rate (red) and sum of the others is α particle event rate.

3.1.2. Random coincidence rate of two^{100}Mo 2νββ decays

The 2νββ decay in a CMO approaches zero rate at the end-point energy, 160 but random coincidence of these events can sum together (pileup) creating backgrounds for the 0νββ signal. The random coincidence of two^{100}Mo 2νββ decays in an energy range, ΔE, can be expressed as [19],

R_{rc} = τ · R^2_0 · ε = τ

( ln2 N T^{2ν2β}_{1/2}

)_2 ε, (1)

where τ is a time resolution, R_0 is a decay rate, N is the number of^{100}Mo decays and ε is the probability of appearing events in the ΔE interval, which was 165 evaluated by convolution of two simulated distributions here. The expected rate of 2νββ decay in a single CMO crystal with ∼306 g is 0.0028 counts/s, which is one double beta decay event per ∼6 mins.

Figure 5: The energy distribution of^{100}Mo 2νββ decays (left) and random coincidences of two 2νββ decays of^{100}Mo (right). The random coincidence spectrum is derived by convolution of the 2νββ spectrum, and normalized according to the 2νββ rate assuming an 0.5 ms coincidence window.

When 5×10^8 2νββ events were simulated in the CMO crystals, ∼99 % of events have energy deposits in one crystal (single-hit events) and the remaining 170 events (<1 %) produced hits in multiple crystals. The random coincidence rate of two 2νββ decays was calculated by convolving two single-hit 2νββ decay energy distributions (see Fig. 5) and the accidental rate in the coincidence window is 1.2 ×10^{−4} ckky in the ROI.

Random coincidence rates of^{100}Mo 2νββ decay and each radioactive back- 175 ground source inside CMO crystals such as^{210}Pb,^{238}U,^{232}Th,^{40}K, and^{235}U are calculated as well. Most concentration values are from the measurements shown in the Table 1, and^{40}K concentration is assumed as 1 mBq/kg [20, 21]. The sum of random coincidence rates from Mo 2νββ decays and other nuclei is 7.80 ×10^{−6} ckky. In the same way, the random coincidence rates of two radioactive 180 background sources inside CMO crystals are calculated and the sum of rates between two background sources are 2.23 ×10^{−8} ckky.

3.2. Backgrounds from materials in detector system 3.2.1. Backgrounds from materials inside and on the cryostat

Activity of radioactive sources in Vikuiti reflector, measured by the HPGe at 185 the Y2L [22], is 0.91 mBq/kg and 0.48 mBq/kg for^{238}U (^{226}Ra) and^{232}Th (^{228}Th), respectively. The CMO supporting copper frame is made of a NOSV grade copper from Aurubis Co. and reported concentration of the NOSV copper [23] is shown in Table 2. We purchased T2FA lead bricks from Lemer Pax with a certified activity of^{210}Pb 0.3 Bq/kg for the inner lead plate and the supercon- 190 ducting lead shield. Activities of^{238}U and^{232}Th in the G10 fiberglass tubes are measured by the ICP-MS, as shown in Table 3, which are in the similar order of the reported results [24]. The activities of^{238}U and^{232}Th in the outer vacuum chamber, made of stainless steel, are from a reference[6], and a measurement of the stainless steel activity is being planned. 195 Table 2: Activities of^{238}U and^{232}Th in Vikuiti reflector [22] and NOSV copper [23]

238U (^{226}Ra)^{232}Th (^{228}Th) Vikuiti Reflector <0.91 mBq/kg <0.48 mBq/kg CMO supporting <16 μBq/kg <25 μBq/kg copper frame

The estimated α and β-α pileup event rates of^{238}U and^{232}Th contaminants in the Vikuiti reflector are in the order of 10^{−4} ckky. But they can be rejected by the PSD analysis like those internal background events. The β-like event rate is in the order of 10^{−4} ckky in the ROI. The estimated α and β-α pileup event rate in the CMO supporting copper frame are in the order of 10^{−5} ckky. 200 Since each crystal is surrounded by the Vikuiti reflector except the top center area, α-particles and βs from the CMO supporting copper frame rarely reach to crystals directly and β-like events, mostly γ-rays, make signals on crystals, as shown in Fig. 6.

Table 3: Concentrations and activities of radioactive sources in materials inside and on the cryostat

210Pb^{238}U^{232}Th Superconducting 0.3 Bq/kg 1 ppt 1 ppt lead shield Cu plate - <16 μBq/kg <25 μBq/kg under inner lead Inner lead plate 0.3 Bq/kg 1 ppt 1 ppt G10 fiberglass tubes - 1,732 ppb 12,380 ppb Stainless steel shield <0.2 mBq/kg <0.1 mBq/kg Outer lead shield <59 Bq/kg 6.9 ppt 3.8 ppt

The effect of radioactive sources from the superconducting (SC) lead shield 205 and other materials, placed out side of the SC lead shield, are from β-like events, mainly γs, like the CMO supporting copper frames. When no events are found in the ROI for a few thousand years of exposure, an upper limit (90% C.L.) is estimated and the limit is to be in the order of 10^{−5} ckky by increasing statistics, as shown in Fig. 7. 210 Random coincidence rates of β-like events from materials inside the cryostat with^{100}Mo 2νββ decay are in the order of ∼10^{−7}−10^{−9} ckky for CMO supporting copper frame, SC lead shield, Cu plate, internal lead plate, which are less than the random coincidence rate of two^{100}Mo 2νββ decays inside the crystals.

3.2.2. Backgrounds from lead shielding box outside the cryostat 215 A major concern of the lead shielding box is the random coincidence events between^{100}Mo 2νββ decay and γs from^{210}Pb, which are enclosed in the 16 tons of the lead shield box. For the lead shielding box, the JR Goslar lead bricks are purchased with a^{210}Pb certification and measured activities of^{238}U and 232Th by the ICP-MS are listed in Table 3. As expected, no events are found in 220

Figure 6: Deposited energy of single hit events from β decay chain (blue) and all decay chains including surface α (red) in CMO crystals originated from^{238}U and 232Th in (a,b) Vikuiti reflector and (c,d) CMO supporting copper frame.

the ROI for 2845 and 352 years of exposure for^{238}U and^{232}Th, respectively. For a^{210}Pb source, 3.3 ×10^{−7} γ events are expected in the 35 crystals. Considering the^{210}Pb activity of ∼59 Bq/kg in the outer lead shield, 2.6 ×10^4 γ events were expected a day and the estimated random coincidence rate is 3.4 ×10^{−6} ckky. The total random coincidence rate of^{100}Mo 2νββ decay for^{210}Pb,^{238}U, 225 and^{232}Th from the outer lead shield is 3.6 ×10^{−6} ckky.

3.3. Backgrounds from rock material surrounding underground laboratory Similar to the lead shielding box, the random coincidence effect of^{100}Mo 2νββ decay and γs from the rock are investigated with reported concentrations of 238U and^{232}Th in rocks at the Y2L [25]. The concentration of^{40}K is 2.44 ppm, 230 calculated with the natural abundance of K in rocks and natural abundance ratio of^{40}K. As expected, no events are found in the ROI and the estimated

Figure 7: Background β-like event rates from^{226}Ra and^{232}Th in the ROI from the cryostat and shielding materials.

upper limits (90% C.L.) are 3.3 ×10^{−7} and 3.7 ×10^{−7} ckky. The total random coincidence rate of^{100}Mo 2νββ decay with γ-rays from^{238}U,^{232}Th, and^{40}K is 9.2 ×10^{−5} ckky. 235 3.4. Other backgrounds

• The sandwich panel and cement floor are ones of candidates with relatively high radioactive sources and huge material mass. Concentrations in samples of laboratory wall, called sandwich panel, and a cement floor was measured by the ICP-MS and listed in Table4. Similar to the effect of rock 240 and the lead shielding box, only γs make hits on crystals. For instance, for the^{232}Th sources from sandwich panel and cement floor, only 7.4 ×10^{−7}% events and 9.6 ×10^{−7}% events appeared, respectively, and no events are in the ROI. The estimated random coincidence rate of^{100}Mo 2νββ decays is in the order of 10^{−6} ckky. 245

Table 4: Concentrations in materials from laboratory environment

238U^{232}Th^{40}K sandwich panel 1.51 ppm 1.25 ppm 202 ppt cement floor 2.14 ppm 8.57 ppm 774 ppt

• Other sources of background (cosmogenic^{88}Y, residual^{48}Ca in the CMO crystals, and^{214}Bi in the copper) are not expected to contribute significantly to the background near^{100}Mo 0νββ decay signal region. Nevertheless, they will be considered in the future.

4. Results 250 The backgrounds estimates of the AMoRE-I for possible radioactive sources are summarized in Table 5. The most dominant background source is internal backgrounds in CMO crystals. After applying rejection cuts such as α-tagging method and PSD, β-like event rate from CMO internal background is reduced to <5.4 ×10^{−5} ckky and <8.3 ×10^{−4} ckky for^{238}U and^{232}Th decay chains, 255 respectively. Vikuiti reflectors and CMO supporting copper frames are the next dominant sources to crystals. After β-α event rejection and^{208}Tl β rejection methods are applied, the event rate is reduced to <1.1 ×10^{−4} ckky and <1.9 ×10^{−4} ckky for^{238}U and^{232}Th, respectively, in the Vikuiti reflector. The event rate with the rejection method in the CMO supporting copper frame is <2.3 260 ×10^{−6} ckky and <2.6 ×10^{−4} ckky, for^{238}U and^{232}Th, respectively. In the end, the total expected rate in the ROI due to direct background sources is <1.5 ×10^{−3} ckky.

Estimated random coincidence rates listed in Table 6 are random coincidence rate of two^{100}Mo 2νββ decays, as well as that of^{100}Mo 2νββ decays 265 with other radioactive background sources from possible background sources, including CMO crystals, Vikuiti reflector, CMO supporting copper frames, G10 fiberglass tubes, outer lead shield, rock shell, etc. The most dominant source

Table 5: Summary of α and β-decay-induced (β-like) backgrounds in major components estimated with measurements and simulation. 99.9999% alpha rejection and 90% β-α rejection are assumed.

Isotopes

Simulated

Backgrounds in ROI Background Time

[×10^{−3} cnt/keV/kg/yr] sources [Years] α β/γ β-α events events events pileup with cuts

Internal

210Pb 44 17 - - -

CMO 238U 34 4.5 - - - 226Ra 520 0.81 0.036 0.19 0.054 232Th 700 <0.55 <31 <0.15 <0.83 235U 68 5.5 - - Vikuiti^{238}U 2.3×10^4 11 <0.041 <0.66 <0.11 reflector^{232}Th 4.7×10^4 4.3 <0.17 <0.18 <0.19 CMO supporting^{238}U 9.9×10^3 0.013 <0.0022 <0.0013^* <0.0023 copper frame^{232}Th 5.7×10^3 0.020 <0.26 <0.0008 <0.26 SC^{238}U 2.6×10^4 - <0.013 <0.013 lead shield^{232}Th 8.4×10^4 - <0.0022 <0.0022 Inner^{238}U 1.5×10^3 - <0.0074^* <0.0074 lead shield^{232}Th 1.2×10^3 - <0.0092^* <0.0092 Cu plate^{238}U 8.7×10^3 - <0.0013^* <0.0013 under lead^{232}Th 2.5×10^4 - <0.0023 <0.0023 G10^{238}U 2.4×10^4 - 0.0026 0.0026 fiberglass tubes^{232}Th 2.5×10^4 - 0.0064 0.0064 Stainless^{238}U 5.3×10^6 - <0.0049 <0.0049 steel^{232}Th 2.6×10^6 - <0.0057 <0.0057 Total <44 <32 <1.2 <1.5

* 90% C.L. with zero-entry

for the random coincidence rate is two^{100}Mo 2νββ decays inside the CMO crystals, 1.2 ×10^{−4} ckky. The next dominant background source for the random 270 coincidence rate with^{100}Mo 2νββ decay is γ from rock shell, due to its huge mass. The total estimated random coincidence rate of^{100}Mo 2νββ decay with backgrounds is <2.3 ×10^{−4} ckky.

Table 6: Backgrounds due to random coincidence with^{100}Mo 2νββ decay

Material Sources

Random coincidence rate [×10^{−3} cnt/keV/kg/yr]

Internal CMO two^{100}Mo 2νββ decays 0.12 210Pb,^{226}Ra,^{232}Th,^{40}K,^{235}U <0.0078 two radioactive sources <2.2 ×10^{−5} Vikuiti reflector^{238}U,^{232}Th <1.1×10^{−5} CMO supporting_{238} U,^{232}Th <3.1 ×10^{−5} copper frame SC lead shield^{210}Pb,^{238}U,^{232}Th <5.8×10^{−4} Cu Plate^{238}U,^{232}Th <5.8×10^{−6} Inner lead shield^{210}Pb,^{238}U,^{232}Th <5.0×10^{−6} G10 fiberglass tubes^{238}U,^{232}Th 4.1×10^{−4} Outer lead shield^{210}Pb,^{238}U,^{232}Th <0.0036 Cement floor 2.61 MeV γ (^{232}Th) 0.0017 Sandwich panel 2.61 MeV γ (^{232}Th) 0.0016

γ from Rock

1.76(^{238}U), 2.61 (^{232}Th) 0.092 1.46 MeV (^{40}K) Total <0.23

5. Discussion

The most dominant background source in the ROI is βs from the^{208}Tl decay 275 in^{232}Th chain inside CMO crystals. In this estimation, the^{232}Th activity inside crystals, 50 μBq/kg, is originated from the upper limit for crystal growing. In reality, activities of^{238}U and^{232}Th inside each crystal are different, so measured activities of each crystal will be used for future work.

For a future experiment after the AMoRE-I, reducing the effect of^{208}Tl de- 280 cay inside crystal is the most important. Therefore, purification of CMO power and its growing process studies are ongoing. In addition, methods for improving α-tagging efficiency for rejecting^{208}Tl have been studied using a simulation. When the internal background level is reduced to the order of 10^{−4} ckky, reducing background effect from radioactive sources from Vikuiti reflector and CMO 285 supporting copper frames should be considered as well.

6. Conclusion

We simulated possible internal and external background sources in the AMoRE- I experiment configuration and the estimated total background rate in ROI is <1.5 ×10^{−3} ckky. The estimated background level shows that the AMoRE-I 290 experiment will achieve the aimed level of 2 ×10^{−3} ckky. For the AMoRE-I, the main background source is βs from^{208}Tl events inside the crystals and materials nearby crystals. In order to reduce background rate further, R&D works for crystal purification and material selection are in progress.

Acknowledgments 295 This research was funded by the Institute for Basic Science (Korea) under project code IBS- R016-D1.

References

[1] R. N. Mohapatra, et al., Theory of neutrinos: A White paper, Rept. Prog. Phys. 70 (2007) 1757–1867. arXiv:hep-ph/0510213, 300 doi:10.1088/0034-4885/70/11/R02.

[2] J. Beringer, et al., Review of Particle Physics (RPP), Phys. Rev. D86 (2012) 010001. doi:10.1103/PhysRevD.86.010001.

[3] C. Giunti, C. W. Kim, Fundamentals of Neutrino Physics and Astrophysics, Oxford, UK: Univ. Pr. (2007) 710 p, 2007. 305 [4] H. Bhang, et al., AMoRE experiment: a search for neutrinoless double beta decay of Mo-100 isotope with Ca-40 MoO-100(4) cryogenic scintillation detector, J. Phys. Conf. Ser. 375 (2012) 042023. doi:10.1088/1742-6596/375/1/042023.

[5] V. Alenkov, et al., Technical Design Report for the AMoRE 0νββ Decay 310 Search ExperimentarXiv:1512.05957.

[6] D. R. Artusa, et al., Exploring the Neutrinoless Double Beta Decay in the Inverted Neutrino Hierarchy with Bolometric Detectors, Eur. Phys. J. C74 (2014) 3096. arXiv:1404.4469, doi:10.1140/epjc/s10052-014-3096-8.

[7] J. W. Beeman, et al., A next-generation neutrinoless double 315 beta decay experiment based on ZnMoO_4 scintillating bolometers, Phys. Lett. B710 (2012) 318–323. arXiv:1112.3672, doi:10.1016/j.physletb.2012.03.009.

[8] D. M. Chernyak, F. A. Danevich, A. Giuliani, M. Mancuso, C. Nones, E. Olivieri, M. Tenconi, V. I. Tretyak, Rejection of randomly coinciding 320 events in ZnMoO_4 scintillating bolometers, Eur. Phys. J. C74 (2014) 2913. arXiv:1404.1231, doi:10.1140/epjc/s10052-014-2913-4.

[9] The 3m enhanced specular reflector film.

URL http://www.3m.com/3M/en_US/company-us/all-3m-products/~/3M-Enhanced-Specular-Reflector-3M-ESR-?N=5002385+8709318+8709341+8710654+8710739+8711017+8712789+8718458+3293061534&rt=rud

[10] H. J. Lee, J. H. So, C. S. Kang, G. B. Kim, S. R. Kim, J. H. Lee, M. K. 325 Lee, W. S. Yoon, Y. H. Kim, Development of a scintillation light detector for a cryogenic rare-event-search experiment, Nucl. Instrum. Meth. A784 (2015) 508–512. doi:10.1016/j.nima.2014.11.050.

[11] S. Agostinelli, et al., GEANT4: A Simulation toolkit, Nucl. Instrum. Meth.

A506 (2003) 250–303. doi:10.1016/S0168-9002(03)01368-8. 330 [12] O. A. Ponkratenko, V. I. Tretyak, Yu. G. Zdesenko, The Event generator DECAY4 for simulation of double beta processes and decay of radioactive nuclei, Phys. Atom. Nucl. 63 (2000) 1282–1287, [Yad. Fiz.63,1355(2000)]. arXiv:nucl-ex/0104018, doi:10.1134/1.855784.

[13] F. Alessandria, et al., Validation of techniques to mitigate copper 335 surface contamination in CUORE, Astropart. Phys. 45 (2013) 13–22. arXiv:1210.1107, doi:10.1016/j.astropartphys.2013.02.005.

[14] G. B. Kim, et al., A CaMoO4 Crystal Low Temperature Detector for the AMoRE Neutrinoless Double Beta Decay Search, Adv. High Energy Phys. 2015 (2015) 817530. doi:10.1155/2015/817530. 340 [15] G.-B. Kim, A 0νββ search using large scintillating crystal with metallic magnetic calorimeter, Ph.D. thesis, Seoul National University (2016).

[16] E. Sala, I. S. Hahn, W. G. Kang, G. W. Kim, Y. D. Kim, M. H. Lee, D. S.

Leonard, S. Y. Park, Development of an underground low background instrument for high sensitivity measurements, Journal of Physics Conference 345 Series 718 (6) (2016) 062050. doi:10.1088/1742-6596/718/6/062050.

[17] F. Alessandria, et al., CUORE crystal validation runs: results on radioactive contamination and extrapolation to CUORE background, Astropart. Phys. 35 (2012) 839–849. arXiv:1108.4757, doi:10.1016/j.astropartphys.2012.02.008. 350 [18] in preparation.

[19] D. M. Chernyak, F. A. Danevich, A. Giuliani, E. Olivieri, M. Tenconi, V. I.

Tretyak, Random coincidence of 2nu 2beta decay events as a background source in bolometric 0nu 2beta decay experiments, Eur. Phys. J. C72 (2012) 1989. arXiv:1301.4248, doi:10.1140/epjc/s10052-012-1989-y. 355 [20] P. Belli, et al., New observation of 2beta 2nu decay of Mo-100 to the 0+(1) level of Ru-100 in the ARMONIA experiment, Nucl. Phys. A846 (2010) 143–156. doi:10.1016/j.nuclphysa.2010.06.010.

[21] D. Blum, et al., Search for gamma-rays following beta beta decay of Mo-100 to excited states of Ru-100., Phys. Lett. B275 (1992) 506–511. 360 doi:10.1016/0370-2693(92)91624-I.

[22] in preparation.

[23] M. Laubenstein, G. Geusser, Cosmogenic radionuclides in metals as indicator for sea level exposure history, Appl. Rad. Isot. 67 (2009) 750. doi:10.1016/j.apradiso.2009.01.029. 365 [24] A. R. Smith, D. L. Hurley, Gamma spectrometric analyses of materials, SNO Technical Reports Rad SNO-STR-91-015 (1991). URL http://www.sno.phy.queensu.ca/sno/str/index.html

[25] M. Lee, et al., Radon Environment in the Korea Invisible Mass Search Experiment and Its Measurement, J. Kor. Phys. Soc. 58 (2011) 713. 370 doi:10.3938/jkps.58.713.